==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.66.00
==========================================================================
Version: 3.66.0
Release Date: 2018.04.30

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3660.ima with checksum          : 70744152
2. 2b2s3660.ima with MD5 checksum      : FF6E982C47B1F403D12D0FA5436F2411
3. 2b2s3660.ima_enc with MD5 checksum  : 40EC086F4BD8C588802321A39E16B8E4
[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)


[Change]:
1. [Add] TLS 1.0&1.1 enable/disable command
2. [Add] update openssl version to 1.0.2

[Bug Fixed]:
N/A

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.

==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.65.00
==========================================================================
Version: 3.65.0
Release Date: 2018.01.30

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3650.ima with checksum          : 69049D60
2. 2b2s3650.ima with MD5 checksum      : 9451930C28ECE22C5E4098D6FC971535
3. 2b2s3650.ima_enc with MD5 checksum  : 3EFD199511970E5E19775A0175BCB6A6
[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)


[Change]:


[Bug Fixed]:

1. S2BX_S2SX issue: [2018 Q1 Block][REG239] PSU2 Status is ''Critical'' when change Artesyn 800W Platinum into Cold redundancy mode.
2. QSM issue: [QSM 1.8.0.1]QSM don't have 'SDR'' configuration item, but S2S BMC webUI Preserve configuration pages have this item.
3. QSM issue: [QSM1.8.0.1] QSM didn¡¦t have ¡§SDR¡¨ Preserve Configuration item, but S2B BMC webUI has.
4. Redfish issue: [[Redfish/FW 13.48] Comparing the actual feedback Info failed with API Spec. v0.7 under URL ''/redfish/v1/systems/1''.

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.64.00
==========================================================================
Version: 3.64.0
Release Date: 2018.01.15

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3587.ima with checksum          : 6909EF07
2. 2b2s3587.ima with MD5 checksum      : 0C7DB61AA75A22FBB3B15DFA9011C1F9
3. 2b2s3587.ima_enc with MD5 checksum  : 8C2DA8B49D4E229BB5203419BEF71984
[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)


[Change]:


[Bug Fixed]:
1. S2BX_S2SX issue: 218317, [2018 Q1 Block] The fan duty weight of Mellanox ON 10GbE CX3PRO (3MS2BLB0000) LAN card is incorrect. (Please refer atttached file 17906.xlsx)

1. S2BX issue: 199971, [2017 Q1 Block] BMC WebUI can not detect correct temperature of Intel PCI-E SSD P3520

2. S2BX issue: 207798, [2017 Q3 Block][REG184]The BMC web UI can't read the Intel SSD DC P4600 series's temperature.

3. S2BX issue: 219134, [OOB 1733]The M10 GPU card find temperature too high BMC event log during GPU stress for S2BV 

4. S2BP issue: 207752, [2017 Q3 Block][REG14]The BMC web UI can't read the Intel SSD DC P4600 series's temperature.

5. S2BX_S2SX issue: 222838, [2018 Q1 Block][REG247] ''Preserve ME Region'' feature item still display on WEBUI when update BIOS FW.

6. S2BX_S2SX issue: 220803, Hex-STRING as result on Snmpwalk -v2c -c , it should be txt string?


[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.63.00
==========================================================================
Version: 3.63.0
Release Date: 2017.11.27

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3587.ima with checksum          : 6AAFD593
2. 2b2s3587.ima with MD5 checksum      : 0C9C7B10B64F31BEBF3DD0E2863DB855
3. 2b2s3587.ima_enc with MD5 checksum  : 724EBFD005FA973A38CA6E7A33C17BB5
[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)


[Change]:


[Bug Fixed]:
1. S2BX_S2SX issue: 217270, SNMP's hddInFailedArray shows unconfigured Bad HDD not critical array. 

1. S2BX_S2SX issue: 217269, SNMP's hddInCriticalArray shows unconfigured Bad HDD not critical array. 

1. S2BX_S2SX issue: 217292, The HDD display unconfigured Bad HDD, but hddDriveFault and hddPredictiveFailure have same result, please help to clarify which information is correct.

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.62.00
==========================================================================
Version: 3.62.0
Release Date: 2017.11.07

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3587.ima with checksum          : 6AAAAA18
2. 2b2s3587.ima with MD5 checksum      : E99EB88C3DCB96A692B615981D74DC62
3. 2b2s3587.ima_enc with MD5 checksum  : 73F27FF5FAD7B78C14B52A6E4E224D02
[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)


[Change]:


[Bug Fixed]:
1. S2SX issue:  Fix the failure in reading data from  HDD Status table via SNMP.

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.61.00
==========================================================================
Version: 3.61.0
Release Date: 2017.10.26

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3587.ima with checksum          : 6AACC6FE
2. 2b2s3587.ima with MD5 checksum      : CA6C0D668257B438E7FA5537C684C747
3. 2b2s3587.ima_enc with MD5 checksum  : BD7465813D6769D305562B561C1D52B7
[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)


[Change]:
1. Change the PSU CR mode.
   PSU0: Active Mode => Master Mode
   PSU1: Standby Mode => Slave Mode

[Bug Fixed]:
1. S2BX_S2SX issue: 212157, Intel 25G XXV710-DA2 is Worst card(FSC Weight is 1.8), but BMC is detect to Normal card(FSC Weight is 1). 

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.60.00
==========================================================================
Version: 3.60.0
Release Date: 2017.10.16

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3587.ima with checksum          : 6AB4E5EE
2. 2b2s3587.ima with MD5 checksum      : 9D3132B78575D9EA68339A576C9C7BB2
3. 2b2s3587.ima_enc with MD5 checksum  : 470430B421C8A6174E13F741F37C4B9E
[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)


[Change]:
1. Add support for monitoring HDD device information by SNMP.

[Bug Fixed]:


[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.59.00
==========================================================================
Version: 3.59.0
Release Date: 2017.09.22

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3587.ima with checksum          : 6AB764F8
2. 2b2s3587.ima with MD5 checksum      : 43ED9B93A5519AC167D889081B526361
3. 2b2s3587.ima_enc with MD5 checksum  : 76DDC0DDF074D0755B92525AF658CB4C

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)


[Change]:
1. Add support for P4500/P4600 temp monitoring

[Bug Fixed]:
1. S2BP issue: 200212/177330, BMC WebUI had drive fault log after power cycle or reboot.
2. S2BP issue: 207552, The BMC web UI can't read the Intel SSD DC P4600 series's temperature.
3. S2B issue: 207798, The BMC web UI can't read the Intel SSD DC P4600 series's temperature.

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.58.00
==========================================================================
Version: 3.58.00
Release Date: 2017.07.07

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3580.ima with checksum          : 6AE698B1
2. 2b2s3580.ima with MD5 checksum      : C27EEA789395F642D02A822818A8CB52
3. 2b2s3580.ima_enc with MD5 checksum  : ED80410483B9CCD9662A3E24BF022360

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)


[Bug Fixed]:
 1.S2S issue:200560, Fix BMC selftest would fail.  
 2.S2BX_S2SX issue:205035/204417, add event filter of voltage and FAN when flashing BMC FW or AC cycle system.
   And turn off SMASH when flashing BMC FW.  

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.57.00
==========================================================================
Version: 3.57.00
Release Date: 2017.06.19

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3570.ima with checksum          : 6AE1980A
2. 2b2s3570.ima with MD5 checksum      : 08F3B48C77FF689F85C6A69176010A57
3. 2b2s3570.ima_enc with MD5 checksum  : 6710F374153000F72C372FFED90633F6

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)


[Bug Fixed]:
 1.S2BX_S2SX: 202634 -Modified the Front Panel Temp_sensor(#0xee)'s retry reading value to avoid  abnormal sensor reading. 

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.56.00
==========================================================================
Version: 3.56.00
Release Date: 2017.06.16

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3560.ima with checksum          : 71B6394D
2. 2b2s3560.ima with MD5 checksum      : A92A1DB7599971BB671230FC8CCB2828
3. 2b2s3560.ima_enc with MD5 checksum  : C494B2BE8822C4172C4E434E67BE22C7

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
1. Added setting PID weight=2.2 when detect MCX_50G_OCP card for all SKU.

[Bug Fixed]:
 

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.

==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.55.00
==========================================================================
Version: 3.55.00
Release Date: 2017.06.05

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3550.ima with checksum          : 6AED7FFD
2. 2b2s3550.ima with MD5 checksum      : D8235DE93A774B8F948B4640553D4706
3. 2b2s3550.ima_enc with MD5 checksum  : A9C733F0D4CE1B701DE222BAD3E2FEC2

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)

[Bug Fixed]:
1. S2BP:203621 changed new system mac address for snmp/smash 

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.

==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.54.00
==========================================================================
Version: 3.54.00
Release Date: 2017.04.06

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3540.ima with checksum          : 6AED7FFD
2. 2b2s3540.ima with MD5 checksum      : D8235DE93A774B8F948B4640553D4706
3. 2b2s3540.ima_enc with MD5 checksum  : A9C733F0D4CE1B701DE222BAD3E2FEC2

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2S         1. Added OCP FRU for OCP card.

[Bug Fixed]:
S2S:        196317 - [2017_Q1_block][Reg29] OCP Mezz ON 25G CX4 FRU update failed.(VRC:97060)
S2SP Plus:  199020 - [REG14] H8 debug port reports incorrect HDD number and weight when the node is with one 82599ES Mezz card and 2 INTEL P3520 PCIE SSD. 
SMS01:      195573 - The interface type of LAN device on S2BP should be displayed in the inventory of QSM, e.g. LOM, OCP
            196036 - The interface type of LAN device on S2B should be displayed in the inventory of QSM, e.g. LOM, OCP
            196268 - S2S Interface device name in QSM should same as BMC Web.

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.

==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.53.00
==========================================================================
Version: 3.53.00
Release Date: 2017.03.28

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3530.ima with checksum          : 6AE3F9DB
2. 2b2s3530.ima with MD5 checksum      : A55A0371528E09786A289F632FD6B01E
3. 2b2s3530.ima_enc with MD5 checksum  : 95CE669703C4E248D983A20A464C08E8

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2BX         1. Update thermal data and fan tables for GPGPU P4.
S2BX_S2SX    2. Update Java certification for remote KVM console till March, 8, 2020.

[Bug Fixed]:
S2BP:      195594 - BMC WebUI can't be displayed the PSU2 Firmware and MFR version when PSU insert in slot 2

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.

==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.52.00
==========================================================================
Version: 3.52.00
Release Date: 2017.01.18

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3520.ima with checksum          : 6AE7ABFD
2. 2b2s3520.ima with MD5 checksum      : C3FB72E60B3DB4E62B61749D12FC6055
3. 2b2s3520.ima_enc with MD5 checksum  : C0302991FC7BBFB8C1DA3D9B6127264C

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2BX_S2SX    1. Resolve CVE-2016-5195.
S2BX         2. Improve to get temperature from Nvida GPGPU device. 

[Bug Fixed]:
S2B:       190784 - sweet32 attack.
           190224 - DNS does not registered when set to Share NIC.
S2S:       170315 - [S2S/BDW/DVT]The temp of NVMeSSD_x sensor, it shouldn\A1\A6t display on S2S BMC Webui (sensor\A1\A6s for S2SP+ only)
           194374 - After changing IPV6 IP Address Source,BMC Web UI can't be log in from IPV6 or IPV4.
           194416 - Correctable ECC / SBE Warning Threshold severity is information which is not the same as eventlog table definition.
           191310 - After post end,QSM can not display CPU,HDD Data and redundant MAC address.
S2BP:      189881 - Run FIO stress test 12 hrs, BMC SEL record ''PSU1 Upper Critical/Upper Non-Critical - Going High'' asserted/deasserted event.
           189274 - BMC FW upgrade with Yafuflash failed with segmentation fault
           182190 - BMC becomes out of service.
           181576 - BMC sensor group read failures.

eTrack ID for RedFish:
           190511 - The threshold value of Volt_P1V05 didn't sync the actual BMC FW under URL ''GET Chassis/1/Power/Voltages/3''. 
           190483 - The BMC will record the power cycle SEL ''Power off/down | Asserted/Deasserted'' after perform the system graceful restart via curl tool.
           190462 - (1) The Redfish will response ''Not Support'' when OSWatchdogPolicy was under ''Do Nothing'' and ''Power Cycle'' mode. (2) The format of Key/Value need to be sync with API Spec. and use the capital letter for ''OS''.
           190460 - Please help to confirm that the string definition of Operation System will be the ''OS'' or ''O/S'' under URL ''PATCH /redfish/v1/Systems/1/Bios/OSWatchdogPolicy''.
           190447 - The actual feedback didn't match with API Spec. under URL ''GET /redfish/v1/Systems/1/Bios/OSWatchdogTimeout''.
           190446 - The actual feedback didn't match with API Spec. under URL ''GET /redfish/v1/Systems/1/Bios/OSWatchdogTimer'' and ''PATCH /redfish/v1/Systems/1/Bios/OSWatchdogTimer''.
           190442 - The actual feedback didn't match with API Spec. under URL ''GET /redfish/v1/Systems/1/Bios/PwrPerfProfile'' and ''PATCH /redfish/v1/Systems/1/Bios/PwrPerfProfile''.
           190438 - The actual feedback didn't match with API Spec. under URL ''PATCH /redfish/v1/Systems/1/Bios/VT-d''.
           190435 - The actual feedback didn't match with API Spec. under URL ''GET /redfish/v1/Systems/1/Bios/VT-d''.
           190421 - The MemoryFrequency always keep on Auto mode after perform the ''PATCH /redfish/v1/Systems/1/Bios/MemoryFrequency''.
           190406 - Some settings didn't work under URL ''Systems/1/BIOS/RASMode''.
           190401 - The HTTPS service was crashed after create the new session via curl tool.
           190368 - The response of Accounts/0 should be the same as Accouts/11 because both of them are invaild values.
           190365 - The HTTPS service was crashed when add new user account with white space or lots of input data.
           190363 - (1) The least and maximum of Username/Password were not follow with BMC Std. Spec. (2) The value of access should not let user to input invalid value.
           190357 - The HTTPS service was crashed when delete user account 0 and over 11.
           190352 - The HTTPS service was crashed when user account's quantity added over 10.
           190288 - (1) Unable to delete the new session via DELETE ''/redfish/v1/SessionService/Sessions/[num]''. (2) The Redfish need to reject the request when user input invalid or empty data.
           190228 - The Redfish is able to let user to input invalid and empty data under POST ''/redfish/v1/EventService/SubScriptions''.
           190223 - Comparing the actual feedback Info failed with API Spec. v0.7 under URL ''/redfish/v1/EventService/SubScriptions/1''.
           190086 - The HTML service was crashed during Redfish stress test under broadcast storm enviroment.

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.

==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.51.00
==========================================================================
Version: 3.51.00
Release Date: 2016.11.17

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3510.ima with checksum          : 6AF995BE
2. 2b2s3510.ima with MD5 checksum      : E5FC1BDEAC0DA55956019F752E40EB38
3. 2b2s3510.ima_enc with MD5 checksum  : 7BD870A1746052414879A1665A98F320

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2BX_S2SX      1. Support remote BIOS configuration specification v1.4.
S2BX_S2SX      2. Support OEM Set/Get active directory configuration commands.
S2BX_S2SX      3. Support OEM Set/Get KVM/Media configuration commands.
S2BX           4. Add power control feature on Java console.
S2BX           5. Support GPGPU P4, P100, M4, M40, M60, 7220P and 7220A.
S2BX_S2SX      6. Add Seagate Nytro XP7200 into worst card table.
S2BX_S2SX      7. correct memory leak issue on rsync service.
S2B            8. Support two GPGPU temperature sensors on S2B SKU 3/4.
S2B            9. Support one GPGPU temperature sensor on S2B SKU 0/1/2/5.
S2BX_S2SX      10.Forbid updating BIOS FW via WEBUI or YAFUFLASH if BIOS NVRAM size is not matched between BIOS flash ROM and BIOS image file.

[Bug Fixed]:
S2S:       180340 - [OOB886] (Redfish v1 BMC FW 3.43) The SUT could be reset even set the wrong request data to Redfish via URI /redfish/v1/Systems/1/Actions/ComputerSystem.Reset.
S2B:       180337 - [Redfish] The SUT could be reset even set the wrong request data to Redfish via URI /redfish/v1/Systems/1/Actions/ComputerSystem.Reset.
S2B:       187809 - [OOB-1328] After install CentOS 7.2, BMC log Unspecified event : ''OS Boot - Invalid Offset for this SensorType''.
S2SR:      183899 - [OOB1062 REG31] The instance value of some sensor doesn't match with BMC spec v.042 define.

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.

==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.50.00
==========================================================================
Version: 3.50.00
Release Date: 2016.07.04

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3500.ima with checksum          : 6B12CE56
2. 2b2s3500.ima with MD5 checksum      : F506904FB8CCE715FA007B17031FA09A
3. 2b2s3500.ima_enc with MD5 checksum  : 47B5744FCA622BDCED6632068147694A

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2BX       1. Updated the weight data of worst card from thermal team on S2B 2U and S2BV system.
S2BX       2. Supported Nvidia Tesla M4 GPGPU.
S2BX       3. Only supported one GPGPU temperature sensor on S2B SKU0/1/2/3/4/5.
S2BX       4. Supported NvMe SSD LED control on S2B 1U SK2 and S2B 2U SKU 3/4/5.
S2SX       5. Added fan present sensors.
S2BX_S2SX  6. Added 'Tesla M4 GPGPU' into worst card table.

[Bug Fixed]:
S2BX_S2SX  1. Correct RedFish API issues.
S2BX_S2SX  2. Failed to update BMC FW through YAFUFLASH when BMC VLAN is enabled.
S2BP:      182539 - After install RHEL7.2, BMC log Unspecified event : ''OS Boot - Invalid Offset for this SensorType-Assert''
S2BP:      171432 - [Q4 Block-REG22][BMC 3.38] There are two unspecified OS boot events(#0x7, #0x8 sensor) during RHEL 7.1 installation.

[Known issue]:
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.

==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.49.00
==========================================================================
Version: 3.49.00
Release Date: 2016.06.21

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : 3AXX / 3B05 or latter.
   S2BP                 : 3AXX / 3B05 or latter.
   S2S/S2SR/S2SP Plus   : 3AXX / 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3490.ima with checksum          : 6C5BE0D0
2. 2b2s3490.ima with MD5 checksum      : C9CA9B13440B9637C8A7267265E0483B
3. 2b2s3490.ima_enc with MD5 checksum  : 6CC219E970BA0B97804C0838F72F3424

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2BX_S2SX  1. Update DRAM setting on boot-loader.
S2BX_S2SX  2. Modify the severity of ECC correctable error event from 'Warning' to 'Information'.

[Bug Fixed]:
S2BX_S2SX  1. Correct RedFish API issues.
S2BX_S2SX  2. Can't update BMC firmware through In-Band script file if user does preserve BMC configurations on updated BMC FW.

[Known issue]: 
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
	   
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.48.00
==========================================================================
Version: 3.48.00
Release Date: 2016.06.02

AMI Subversion Revision: AMI SPX 2011Q3

[Associtate platforms]
1. BIOS	version.
   S2B/S2BV             : S2B 3B05 or latter.
   S2BP                 : S2BP 3B05 or latter.
   S2S/S2SR/S2SP Plus   : S2S 3B07 or latter.
2. X5M Firmware version : 3.35 or latter.

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3480.ima with checksum          : 65E5E0C2
2. 2b2s3480.ima with MD5 checksum      : FB216CEA2F08E97E1145A837E9F6B49D
3. 2b2s3480.ima_enc with MD5 checksum  : D51966F4CC13A8E7164E4E63C8036555

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2B S2SP_PLUS 14. Support NVMe MI SSD LED control function.

[Bug Fixed]:
S2B       Fixed S2B SKU2 DC_on initial NVMe SSD LED control incorrect issue

[Known issue]: 
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.

==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.47.00
==========================================================================
Version: 3.47.00
Release Date: 2016.05.27

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3470.ima with checksum          : 6C6E160C
2. 2b2s3470.ima with MD5 checksum      : 1A54D8119F907D113EF3CD456573283E
3. 2b2s3470.ima_enc with MD5 checksum  : 3FC0898C67390C8044E6F01A8E89921E

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2BX_S2SX     1.  Support RedFish API.
S2BX_S2SX     2.  Support 0x7/0x8/0x9/0xa offset on OS boot sensor type.
S2BX_S2SX     3.  Add SAS MEZZ LSI 3108 into worst card table.
S2BX_S2SX     4.  Upgrade DRAM setting to version 061 on boot-loader.
S2BV          5.  Update thermal coefficient value.
S2SX          6.  Get the POUT MAX and POUT reading from CMC FW due for supporting 1800W PSU.
S2SX          7.  Support 'MB Type Error' event and forbid system DC on if BMC detects MB type error on X5M system.
S2BX_S2SX     8.  forbid the cold reset command to work when BMC is in update mode for updating BMC or BIOS firmware.
S2BX_S2SX     9.  Enable polling mode to replace NCSI AEN if BMC is in Broadcast storm environment.
S2BX_S2SX     10. Support 'On board HDD information' from BIOS based on new OEM HDD command.
S2BX_S2SX     11. Support remote BIOS configuration specification v1.2.
S2BX_S2SX     12. Forbid BIOS FW update to go if the project name is not match between BIOS FLASH ROM and BIOS FW image via YAFUFLASH.
S2BX_S2SX     13. Support VMCLI feature.
S2B S2SP_PLUS 14. Support NVMe MI SSD LED control function.

[Bug Fixed]:
S2BX_S2SX  Fixed CVE-2015-7547 Vulnerability.
S2BP:      178349 - Use Yafuflash utility with wrong BIOS file, SUT can finish flashing BIOS.
           177882 - When BMC update via Yafuflash out band, execute BMC cold reset IPMI command will make BMC dead(HB solid green).
S2S: \A1@ \A1@ 177471 - The BIOS 3B06 can't be updated successfully via BMC WebUI, it will show ''Error: there is a error due to flash write action''
           178429 - [REG 36](Re-Spin)The BMC SEL shows ''SKU - Chassis - Unavailability - Asserted'' after plugging node into node4(S2SP+: 177161)
S2SP Plus: 171833 - Error message ''Critical Interrupt #0xa1 | PCI SERR | Bus Correctable error'' in the SEL log during AC cycle test  
           177533 - [PVT]The Severity of SEL ''[Fan_SYSx_x]: Lower Critical - Going Low - Deasserted'' under mail server is incorrect, it should be ''Info'' not ''Critical''
           177468 - [PVT]The BIOS 3B06 can't be updated successfully via BMC WebUI, it will show ''Error: there is a error due to flash write action''(DOS update successfully)
           177161 - [PVT]The BMC SEL shows ''SKU - Chassis - Unavailability - Asserted'' after plugging node into node4
           176348 - The sensor thresholds of NVMeSSD_0&1 does not match with BMC FW Spec rev041.
S2SR:      171432 - [Q4 Block-REG22][BMC 3.38] There are two unspecified OS boot events(#0x7, #0x8 sensor) during RHEL 7.1 installation.
S2B:       180879 - [S2B CMC] Should not detect CMC version in S2B.

[Known issue]: 
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.

==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.46.00
==========================================================================
Version: 3.46.00
Release Date: 2016.05.11

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3460.ima with checksum          : 6E6C9E10
2. 2b2s3460.ima with MD5 checksum      : 8F2D51AB97526DA1092BBD37C512C32A
3. 2b2s3460.ima_enc with MD5 checksum  : BE0EB65352AB1D9587D4C4164B2E8D44

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2BV  1. Support CJ2 (Valley Vista) card.

[Bug Fixed]:
N/A

[Known issue]: 
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.

==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.45.00
==========================================================================
Version: 3.45.00
Release Date: 2016.04.29

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3450.ima with checksum          : 67F92D12
2. 2b2s3450.ima with MD5 checksum      : 067C9B16A9D1C576F7DBFE096798F07D
3. 2b2s3450.ima_enc with MD5 checksum  : E46C1272C8795131698B015CB408FCA5

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2BX_S2SX  1. Add support Linux32/64 Yafuflash IB BMC flash update function.

[Bug Fixed]:
N/A

[Known issue]: 
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
       
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.44.00
==========================================================================
Version: 3.44.00
Release Date: 2016.04.12

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3440.ima with checksum          : 6E82480F
2. 2b2s3440.ima with MD5 checksum      : E34904197AD962D48B00D6162D8447F5
3. 2b2s3440.ima_enc with MD5 checksum  : 39271F99C7BE8B47C07710B87C59EA59

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2BX_S2SX  1. Add SAS MEZZ LSI 3108 into worst card table.

[Bug Fixed]:
N/A

[Known issue]: 
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	7. to support PSU device 1800W, BMC firmware version would be updated to 3.43 or newer 
       and CMC firmware version would be updated to 3.35 or newer simultaneously.
	   
==========================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP Plus AST2400 BMC FW Release v3.42.00
==========================================================================
Version: 3.42.00
Release Date: 2016.02.05

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3420.ima with checksum          : 6E881FBE
2. 2b2s3420.ima with MD5 checksum      : 87311F80A70EFF4AB891A9494BC60DE9
3. 2b2s3420.ima_enc with MD5 checksum  : DF7056A16D184EE3EDFA791104628EA4

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP Plus)
S2BX_S2SX  1. Corrected the string memory parity event log from "Memory Parity Error" to "Parity" followed with IPMI spec..
S2BX_S2SX  2. Corrected the data offset of processor and memory information in EEPROM from offset 0x2000 to offset 0xc00.

[Bug Fixed]:
S2BX_S2SX  1. Fixed memory leak on WEBUI library while try to login WEBUI with wrong password.

[Known issue]: 
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.
	   
=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.41.00
=====================================================================
Version: 3.41.00
Release Date: 2016.01.28

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3410.ima with checksum          : 6E8A0451
2. 2b2s3410.ima with MD5 checksum      : A18D1F9C0AA984CD79FF49CB7B87BEC4
3. 2b2s3410.ima_enc with MD5 checksum  : 8F662C42D335DD1F62CC94C4B6CB0790

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP/S2SP Plus)
S2BX_S2SX  1. Appended event raw data to trap payload for detail information of trap alert.
S2BX_S2SX  2. processor and memory information stored in EEPROM.
S2BX_S2SX  3. BMC won't send event trap if added lots of PEF settings.
S2BX_S2SX  4. Enhanced error handling with IPMI VLAN function, SNMP service will crash when VLAN is connected and input wrong password.
S2BX_S2SX  5. Adviser service on remote kvm function would crash when it received a invalid network package.
S2BX_S2SX  6. Adviser service has to check if the session is valid and existed before doing specific action.
S2BX_S2SX  7. BMC forbids to update BIOS FW via WEBUI or YAFUFLASH while end user want to preserve BIOS configuration and BIOS NVRAM size on new BIOS FW is not the same with old BIOS FW on BIOS FLASH.
S2BX_S2SX  8. ME FW would produce a SPS FW health event sometimes when upgrade BIOS and ME.
S2SX       9. Corrected Openssl library because TLSv1.0 or TLSv1.1 is not compatible with IE broswer.
S2SX       10. Added slot ID sensor on BMC SDRS for multi-nodes system.

[Bug Fixed]:
S2B:       172301 - [Broadwell CPU] BMC WebUI can not be connected normally, when user disable/enable the IPv6 mode under BIOS utility.
S2S:       173195 - DIMM Temperature sensor will get temperature successfully during POST on S2S
           172092 - [OOB 751](REG 13)(BMC 3.40) It's very slow to open the BMC WebUI (Browser: IE11). (S2SP+: 172116)
		   172012 - [OOB 751](REG 13)(BMC 3.40) RKVM can not be opened via IE 11.0/Google Chrome 47.0.2526.106/FireFox 44.0b1. (Java version is 8u66)
SMS01:     172062 - BMC won't send event trap if add too many PEF settings.

[Known issue]: 
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.40.00
=====================================================================
Version: 3.40.00
Release Date: 2015.12.10

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3400.ima with checksum          : 6EF03789
2. 2b2s3400.ima with MD5 checksum      : 955602F6BB4B51ABD2C104970FA4E9B1
3. 2b2s3400.ima_enc with MD5 checksum  : 9BA2E983433EEA080F3F0F200C334459

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP/S2SP Plus)
S2BX_S2SX  1. Improved SNMP service.
S2BX_S2SX  2. Improved KCS and Ethernet driver modules.
S2BX_S2SX  3. Support TLSv1.1 and 1.2.
S2BX_S2SX  4. Disable all TLS ciphers using less than 128 bits of encryption.
S2BX_S2SX  5. Increase RSA key strength of web to 2048.
S2BX_S2SX  6. Corrected the event string of "Correctable Memory Logging Disabled" sensor on WEBUI.
S2BX_S2SX  7. Disabled IPMI cipher suit ID 0 by default.

[Bug Fixed]:
S2B:       169476 - [Broadwell CPU] Sometimes BMC log 2-3 times event about ''power off - deasserted'' during one time power cycling. 
           170232 - [OOB-646][BMC 3.39 sanity change bug verify for KDDI]''Bug Fixed'' should not have ''N/A'' when there already have list bug fix information in BMC 3.39 readme file.
S2SP Plus: 170454 - BMC sensor name for X5M dual rotor FAN goes FAN_SYS0_1/2, mismatch to Std. SPEC FAN_SYS0_0/1.
           170212 - BMC RKVM mounted virtual DVD and remote network ping lost when stress BMC dedicated-NIC under 9000+ network packets.
		   170024 - Unable to flash the BMC FW via Yafuflash tool v2.26.07 via CMS with ARP.
           169953 - [DVT]The KCS stress under DOS failed after 64 cycles under S2SP Plus(Similar to147576)
		   169692 - BMC event ''BMC hardware watchdog timeout reset'' recorded during SUT warmboot cycling.

[Known issue]: 
N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.
	6. In order to enhance WEB server security, BMC FW is already disabled insecurity SSLv3.
       so far BMC FW version 3.40 start to support TLSv1.1 and TLSv1.2 extra.
       then on remote client environment, user also need enable "TLSv1.1 and TLSv1.2" features on WEB browser accordingly.

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.39.00
=====================================================================
Version: 3.39.00
Release Date: 2015.11.24

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3390.ima with checksum          : 6F9A8E9F
2. 2b2s3390.ima with MD5 checksum      : 67B467CE039AC39A38BCE0790F911344
3. 2b2s3390.ima_enc with MD5 checksum  : CB09E02447D1C56F369ABD379ACE1740

[Change/Add]: (S2BX_S2SX: S2B/S2BV/S2BP/S2S/S2SR/S2SP/S2SP+)
S2BX_S2SX  1. Changed to "not allowed to access rkvm" if seconds user would like to get remote kvm privilege, but first one user doesn't have any action and timeout.
S2BX_S2SX  2. Supports PSU1 in active mode and PSU2 in sleep mode if both of power supply devices with AC input as PSU cold redundant feature enabled.
S2BX_S2SX  3. QSM would show mezzy DIMM information at DIMMA0 on compute node.
S2B        4. Updated coeficient value on one CPU configuration with three dual fan modules.

[Bug Fixed]:
S2B:   167725 - BMC WenUI doesn't work via VLAN on BMC v3.37
S2B:   169764 - [Broadwell CPU] Sometimes BMC log the unknow event about ''0x07'' and ''0x08'' when user power on/off system.

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.38.00
=====================================================================
Version: 3.38.00
Release Date: 2015.10.05

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3380.ima with checksum          : 6F961E66
2. 2b2s3380.ima with MD5 checksum      : 69B3DAF2CCFD05AC4960925B2BFB29AB
3. 2b2s3380.ima_enc with MD5 checksum  : 1B0B673ACC872BFDF06DAAE63A31CA85

[Change/Add]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
S2BX_S2SX  1. Correct memory parity event log on WEBUI.

[Bug Fixed]: N/A

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.37.00
=====================================================================
Version: 3.37.00
Release Date: 2015.09.24

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3370.ima with checksum          : 6F9A0B97
2. 2b2s3370.ima with MD5 checksum      : 01775DAABDC0ED6FE7B869B502C89FE8
3. 2b2s3370.ima_enc with MD5 checksum  : 7F15AC554D140F3956CE789AB2B3B103

[Change/Add]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
S2BX_S2SX  1. Fix memory leak issue on web server.
S2BX_S2SX  2. the message digest algorithm on WEB server is changed from MD5 to SHA1.
S2BV       3. Support TESLA M60 GPGPU.

[Bug Fixed]:
S2B:   165783 - Shows ''CD/DVD: CD Port:5120 is not listening. Closing the CD redirection.'' when connecting iso image as a CD-ROM via BMC Virtual Console.
       160870 - BMC NIC got insecure test result of utility Nessus Vulnerability Scanner(network security), item: Medium severity ''Transport Layer Security(TLS) Protocol CRIME Vulnerability''.
S2S:   164286 - [REG17]BMC WebUI will show PCIe Error SEL ''ManufacturerID:001c4c/VID:010c/DID:00ff/ErrorID 1:0/ErrorID 2.0'' when system occurs DIMM initialization fail/DIMM configuration problem
       164091 - [REG17]The BMC SEL shows error SEL (SPS' FW Health) 'NM(OEM) Firmware Status - Persistent Storage Integrity Error - Asserted'' after update ME FW under Linux.
       165335 - Login BMC WebUi with HTTPS and open RKVM , the system will display ''Unable to launch the application.(Java version 8u60) 
       160873 - [Nessus Vulnerability Scanner Utility] BMC NIC got insecure test result (network security), item: Medium severity ''Transport Layer Security(TLS) Protocol CRIME Vulnerability''.

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.36.00
=====================================================================
Version: 3.36.00
Release Date: 2015.09.01

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3360.ima with checksum          : 7033FA8B
2. 2b2s3360.ima with MD5 checksum      : F4C1DBC166FC55CA1FC34A109D4E4C08
3. 2b2s3360.ima_enc with MD5 checksum  : 2F5B033DBB579CF4F973C470CE90E0A4

[Change/Add]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
S2BX_S2SX  1. Supports to enable/disable the ncsi failed-over function through IPMI command and WEBUI.

[Bug Fixed]:
S2B:   164975 - [S2B 2015 Q3 BMC 3.35] User get SNMP SNMP Community String fail, but the command works when enter BMC WEBUI SNMP Community setting
       163821 - Share NIC 1 will toggle to Share NIC 2 when the system is reset.
S2S:   164306 - [REG17]The SEL for Clear Password by jumper doesn't meet SEL Standard Spec V 1.25.
       164286 - [REG17]BMC WebUI will show PCIe Error SEL ''ManufacturerID:001c4c/VID:010c/DID:00ff/ErrorID 1:0/ErrorID 2.0'' when system occurs DIMM initialization fail/DIMM configuration problem.
       164918 - [REG10]Virtual-media NFS OEM command doesn't work successfully if OS image size is 5 GB under S2S(EMC BMC eTrack: 164907)
	   164907 - [EMC BMC] Virtual-media NFS OEM command doesn't work successfully if OS image size is 5 GB under S2S(for QCT BMC :164918)
	   164589 - [REG10]The BMC 3.34.00 ReleaseNote format doesn't meet BMC Standard format.

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.35.00
=====================================================================
Version: 3.35.00
Release Date: 2015.08.14

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3350.ima with checksum          : 7039975A
2. 2b2s3350.ima with MD5 checksum      : AC633353B6771DE942FC15D12712D734
3. 2b2s3350.ima_enc with MD5 checksum  : 72045AEEF1D915BA7AEBF12EDA31375B

[Change/Add]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
S2BX_S2SX  1. Adds options to preserve BIOS region and ME region on WEBUI.
S2BX_S2SX  2. Always get DIMM temperature from DIMM slot 0.
S2BX_S2SX  3. Supports OEM extended DIMM event log.
S2BX       4. Updates fan tables on S2B 1U and S2BP systems.

[Bug Fixed]:
S2B:   163742 - SEL error report for PSU2 error when system run ambient temperature over 35C, but if, ambient temp at 30C no error report and working fine.
S2BP:  159921 - OOB-354 Intel Quick Assist Adapter 8950] SEL has some Fan_PSU error event during AC cycle with 8950 adapter.
S2S:   164306 - REG17]The SEL for Clear Password by jumper doesn't meet SEL Standard Spec V 1.25

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.34.00
=====================================================================
Version: 3.34.00
Release Date: 2015.08.04

AMI Subversion Revision: AMI SPX 2011Q3

[X5M FW]: For Multi-Nodes system (S2SX: S2S/S2SP/S2SR)
X5M FW Version: v3.22.0 or above

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3340.ima with checksum          : 7050DC1D
2. 2b2s3340.ima with MD5 checksum      : 68260A7E21339B978B7E30B1D2AE3205
3. 2b2s3340.ima_enc with MD5 checksum  : D0F77CE87AC04278A6672870EB3494E1

[Added]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
S2BX_S2SX  1. Adds a type for memory parity error.
S2BX_S2SX  2. Supports Get/Set SSL certificated commands.
S2BX_S2SX  3. Enables User ID 2 to be enabled or disabled.

[Changed]:
S2BX       1. Updates fan tables on S2B 1U and S2BP systems.

[Bug Fixed]:
S2B:   161433 - [BDW-EP]Severity of ''TCC Activation - Asserted'' is information but event log table v1.23 defines as ''Warning''.
S2BP:  159921 - [OOB-354 Intel Quick Assist Adapter 8950] SEL has some Fan_PSU error event during AC cycle with 8950 adapter.
S2S:   163786 - The SEL string for CMOS clear doesn't meet SEL Standard Spec V1.24.
       163825 - The ''Error'' string for Other IIO spells incorrectly, it shows ''Erro'' under BMC WebUI

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.33.00
=====================================================================
Version: 3.33.00
Release Date: 2015.07.01

AMI Subversion Revision: AMI SPX 2011Q3

[X5M FW]: For Multi-Nodes system (S2SX: S2S/S2SP/S2SR)
X5M FW Version: v3.22.0 or above

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3330.ima with checksum          : 70505C40
2. 2b2s3330.ima with MD5 checksum      : 527A9C43EA58DD45B66BB5044DF7515F
3. 2b2s3330.ima_enc with MD5 checksum  : 0C86A06E3B8FA5120F79BA7E2EE3B0C3

[Added]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
S2BX_S2SX  1. Supports CPLD FW update through YAFUFLASH tool.
S2BX_S2SX  2. Always enables HTTPS for WEBUI connection.
S2BX_S2SX  3. Supports the login/logout/login failed/login timeout of WEBUI event logs.
S2BX_S2SX  4. Supports OEM SNMP commands.
S2SX       5. Adds the FW compatible log if CMC and BMC FW are not compatible.
S2SX       6. Forbid updating BMC FW if CMC and BMC FW are not compatible.
S2BX       7. Supports to decide PSU number(s) during BMC boot up once and the default mode is cold redundant if two PSUs are present.

[Changed]:
S2BX_S2SX  1. Updates openssl-0.9.8zf.
S2BX_S2SX  2. Disables CBC Ciphers and weak MACs for SSH server.

[Bug Fixed]: N/A
S2B:   161820 - [BDW-EP] SEL will not log CPU_VR_HOT event when Temp_VR_CPU# sensor has reached UNC threshold then system power off.
       161433 - [BDW-EP]Severity of ''TCC Activation - Asserted'' is information but event log table v1.23 defines as ''Warning''. 
	   160870 - BMC NIC got insecure test result of utility Nessus Vulnerability Scanner(network security), item: Medium severity ''Transport Layer Security(TLS) Protocol CRIME Vulnerability''.
S2BP:  159921 - [OOB-354 Intel Quick Assist Adapter 8950] SEL has some Fan_PSU error event during AC cycle with 8950 adapter.
       156785 - The SOL will disconnect when runing Warmboot Cycling. (Shared-NIC on LOM NIC2)
S2BV:  160592 - [Customer issue]FAN zone is empty(without GPGPU) then FAN speed will be 8xxx~10xxx RPM when populating one GPGPU(K20X) only. (with 2 GPGPU, FAN speed is normal.)
S2S:\A1@ 160873 - [Nessus Vulnerability Scanner Utility] BMC NIC got insecure test result (network security), item: Medium severity ''Transport Layer Security(TLS) Protocol CRIME Vulnerability''.
S2SP:  161801 - [Field] BMC's requesting ip every two mins and not following DHCP lease time. The extra requests result in increased network traffic and logfile size on DHCP server.
SMS01: 159456 - QSM will report 4 times chassis power consumption than real in S2S
SMS02: 159457 - QSM will report 4 times chassis power consumption than real in S2S

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 and CMC FW 3.22 start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or newer is incompatible to X5M FW version 3.21 or older.

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.32.00
=====================================================================
Version: 3.32.00
Release Date: 2015.05.22

AMI Subversion Revision: AMI SPX 2011Q3

[X5M FW]: For Multi-Nodes system (S2SX: S2S/S2SP/S2SR)
X5M FW Version: v3.22.0 or above

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3320.ima with checksum          : 70834F30
2. 2b2s3320.ima with MD5 checksum      : AF3897D03FCAF141FDBB5EC2DB7D077F
3. 2b2s3320.ima_enc with MD5 checksum  : C2EBED955C7BC9474C277E74ACB912F3

[Added]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
S2BX_S2SX  1. Added Seagate XP6302 and Intel Quick Assist Adapter 8950 card into worst card table for fan control.

[Changed]:
S2B1U_S2BP 1. Updated fan tables for Seagate XP6302 card.

[Bug Fixed]: N/A

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
	5. BMC FW 3.26 or above start supporting new X5M protocol version 0.27.
	   Please be noted that BMC FW 3.26 or above is compatible to X5M FW version 3.22 or above.

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.31.00
=====================================================================
Version: 3.31.00
Release Date: 2015.05.08

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3310.ima with checksum          : 70805DA1
2. 2b2s3310.ima with MD5 checksum      : ADC76A2D28792EB7B11F3C48A1F42871
3. 2b2s3310.ima_enc with MD5 checksum  : 5EC99116367948E382B3EDB23BBF9F9E

[Added]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
S2SR      1. Added a OEM command to enable or disable NMI automatic generation.
S2SX      2. Supported new repeater format.
S2SX      3. Added node power reading based on each node status for multi-nodes.
S2BX_S2SX 4. Supported virtual device through NFS server.
S2BX_S2SX 5. Supported BroadWell-EP CPU type.

[Changed]:
S2BX      1. Updated fan tables on S2BP and S2B 1U.
S2BX      2. Corrected the GPGPU status to absent status if any one of GPGPU device is not present.
             then it would avoid fan duty ramping up to maximum duty.
S2SX      3. Updated thermal C values depended on each node status for multi-nodes.

[Bug Fixed]:
S2B:
      160107 - [S2B_BDW] There is no CPU1 info dispalyed of BMC WebUI, but BIOS detect normally.
S2BP:
\A1@\A1@\A1@159921 - [OOB-354 Intel Quick Assist Adapter 8950] SEL has some Fan_PSU error event during AC cycle with 8950 adapter.
S2SR: 
      159557 - [LSI 9361-8i] There are some invalid event logs and warning message on pop-up window on BMC WebUI.

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.30.00
=====================================================================
Version: 3.30.00
Release Date: 2015.03.31

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3300.ima with checksum          : 75648019
2. 2b2s3300.ima with MD5 checksum      : CF2DCDFE0462F0F34C441035EEBA1A7A
3. 2b2s3300.ima_enc with MD5 checksum  : 10C5F57717FDA88081B9562C5058160B

[Added]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
S2BX_S2SX 1. Added the hostname option for DHCP server.
S2B       2. The default value of IPV6 feature is disable for UBR.

[Changed]:
S2BX_S2SX 1. Updated the new QCI logo on WEBUI.
S2BX_S2SX 2. Updated the Storage library.
S2BX_S2SX 3. Updated the Glibc library for Ghostfix issue.
S2BX_S2SX 4. Improved to protect the ncml.conf file.
S2BX_S2SX 5. Changed the procedure of Shared NIC selection.
S2BX_S2SX 6. Fixed the BMC HW watchdog reset due to NCSI failed.
S2BX_S2SX 7. Changed the NCSI timeout to 2 seconds based on NCSI Spec.
S2BX_S2SX 8. PSU Redundancy sensor was changed the behavior polling on DC on and DC off.

[Bug Fixed]:
S2B:
      158773 - [SDA_OOB] There is one HVDC PSU will change to standby mode during AC 120V/230V 50Hz interrupt test.
      158692 - [Q1 Block] The Temperature sensor NVMeSSD_0/1 under BMC Spec maybe rename ''Temp_SSD 0/1'' to meet BMC WebUI.
      158685 - [Q1 Block] The Temp_SSD UNC/UC Temperature doesn't meet BMC Spec.
      158664 - [Q1 Block] The OCP UNC/UC Temperature under BMC 3.19 is incorrect.
      157529 - [Mellanox 40G FDR OCP mezz card] WEBUI couldn't connect from LAN card when BMC sets share-NIC(OCP) and SUT is idle in OS.
S2S:
      157750 - [S2S Reg10/Quarterly Reg] The SEL doesn't show ''Power Supply Input Lost (AC/DC) - Asserted'' and ''Redundancy Lost - Asserted'' after unpluging PSU power cord

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin
		
=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.29.00
=====================================================================
Version: 3.29.00
Release Date: 2015.03.02

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3290.ima with checksum          : 783F4054
2. 2b2s3290.ima with MD5 checksum      : F26E4EB57D3A26C7F4856AA74E1D5CF8
3. 2b2s3290.ima_enc with MD5 checksum  : 89A6A4D24A4E1FA5E5EE32545592A12E

[Added]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
N/A

[Changed]:
S2BP      1. the DIMM information would show incorrectly through SNMP agent.
S2B       2. Changed the sensor name from Temp_PCIE_SSDx to NVMeSSD_x.
S2B_S2BP  3. Updated fan table because thermal has improved the NvMeSSD data.
S2B_S2BP  4. Changed the threshold value of NVMeSSD_x sensor according to Intel or Samsung NvMe SSD.

[Bug Fixed]:
S2BP:
      157701 - [rev.D BP] SEL has some error logs during storage stress with 10 Samsung PCIE SSD.
	  157699 - [rev.D BP] HDD0 ''Drive Presence - Asserted'' and ''Drive Presence - Deasserted'' logged in SEL during stress with 10 INTEL PCIE SSD.
	  
[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2B/S2S/S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.28.00
=====================================================================
Version: 3.28.00
Release Date: 2015.02.12

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3280.ima with checksum          : 78543253
2. 2b2s3280.ima with MD5 checksum      : 0F757F6F632B3F5F4223E7A84A698519
3. 2b2s3280.ima_enc with MD5 checksum  : 89C4B9453BD810B448AC61E99215B333

[Added]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
S2SR  1. Supported to generate NMI signal automatically once BMC detected the AC power failed.

[Changed]: N/A

[Bug Fixed]:
S2SR:
      157409 - [Reg]The FRU Device Description would got \A1\A7AST2300\A1\A8 after use ipmitool by out band (ipmit ver:1.8.13 and it should be AST2400)

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.27.00
=====================================================================
Version: 3.27.00
Release Date: 2015.02.09

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3270.ima with checksum          : 785A60EA
2. 2b2s3270.ima with MD5 checksum      : 2DF91A7A814D37FF68E556949AFACCE4
3. 2b2s3270.ima_enc with MD5 checksum  : 70C9AF2E53AC684370D9A011B017FEF8

[Added]: (S2BX_S2SX: S2B/S2S/S2BV/S2BP/S2SR/S2SP)
S2B         1. Supported OCP temperature sensor based on OCP 2.0 Mezz spec define.
S2SR        2. Supported the second BBU version in WEBUI.
S2BP        3. Added PSU temperature and PSU fan sensors.

[Changed]:
S2BX_S2SX   1. PSU Vin fault status will not be reference to the status of power failed pin if any of power cord is attached.
S2BP        2. Updated fan table.

[Bug Fixed]:
S2SR:
      156999 - [Reg] BMC 3.26 would not report PSU1 or 2 lost and PSU Redundancy event after unplug power cord.
      156519 - [Reg]The node2 would report BBU1 Battery low log, but node1 BMC doesn\A1\A6t find this log while system idle in BIOS BMC network configuration page.
      156513 - [Suggestion]BBU sensor sequence from BBU1 first then show BBU2.
      156547 - [Suggestion]Show BBU1 and BBU2 FW version in BMC WebUI dashboard page.
	  157244 - [Reg]The BMC sensor only record this \A1\A7HDD0 Driver slot(Bay)\A1\A8log after BBU in discharge mode with turn off front HDDs.
	  155216 - [PVT-ALL]The BMC SEL would record this ''Volt_P12V ''log during BBU discharge mode while node1 plug/unplug
      155620 - [PVT-ALL]The node 2 BMC SEL doesn't record HDD0~HDD23 Driver slot(Bay) logs after expander board plug/unplug
	  
[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.26.00
=====================================================================
Version: 3.26.00
Release Date: 2015.01.12

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.11.01)

[Firmware Images]:
1. 2b2s3260.ima with checksum          : 786B4804
2. 2b2s3260.ima with MD5 checksum      : 6CAE62153904E5B57846F794B1C780E5
3. 2b2s3260.ima_enc with MD5 checksum  : 4B6F99B3F6CAB5049C7FBF2BEFAE0868

[Added]: (S2BX_S2SX: S2BV/S2BP/S2SR/S2SP)
S2BX_S2SX   1. Supported BIOS SPI N25Q128A flash.
S2SR        2. Supported second BBU device through X5M sensor exchange. (Compatibly with CMC v3.22.0 or above)
S2SR        3. Supported the S2SR expander specification v0.9.

[Changed]:
S2BX_S2SX   1. Updated the SOCFLASH tool.(version 1.11.01)
S2BX        2. Updated the threshold value of OCP sensor.

[Bug Fixed]:
S2SP:
     155664 - AC cycle test would have RTC check fail at loop 3 (occurred once)
S2SR:
     155570 - [PVT-All] Battery_PSU_STA sensor naming confused to be Battery or PSU.
S2BV:
	 155187 - [SMS02] Inventory data didn't get BIOS version in QDCM.
S2BP:
     155188 - [SMS02] Inventory data didn't get BIOS version in QDCM.

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.25.00
=====================================================================
Version: 3.25.00
Release Date: 2014.12.30

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.09.02)

[Firmware Images]:
1. 2b2s3250.ima with checksum          : 7874267B
2. 2b2s3250.ima with MD5 checksum      : 2BAD751D349468A50A968F0F50D9E15A
3. 2b2s3250.ima_enc with MD5 checksum  : 576A0933A0149E364D867B746E90E01A

[Added]:
S2BX_S2SX  1. Supported OCP temperature sensor based on OCP 2.0 Mezz spec define.
S2BX_S2SX  2. Supported memory module enabled on remote bios configuration protocol.

[Changed]:
S2SR       1. Updated the threshold value of Battery temperature.

[Bug Fixed]:
S2SR:
     154722 - [PVT-ALL]Node 1 doesn\A1\A6t record this \A1\A7Charge Inhibit \A1\A8log in BMC SEL when BBU temp higher than 48 degee while discharge mode(but node 2 has been recorded )
S2BP:
	 155152 - Inventory data didn't get some DIMM S/N and P/N information

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.24.00
=====================================================================
Version: 3.24.00
Release Date: 2014.12.24

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.09.02)

[Firmware Images]:
1. 2b2s3240.ima with checksum          : 7872DF0A
2. 2b2s3240.ima with MD5 checksum      : 9CA847708D105B50E2D20078EDAF684A
3. 2b2s3240.ima_enc with MD5 checksum  : B5E709BD1D83D6067584FA7BC38F6E38

[Added]:
S2SP     1. Supported to control PCIESSD LED. (PCIESSD present: HDD LED on; PCIESSD absent -> HDD LED off)

[Changed]: N/A

[Bug Fixed]: N/A

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.23.00
=====================================================================
Version: 3.23.00
Release Date: 2014.12.22

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.09.02)

[Firmware Images]:
1. 2b2s3230.ima with checksum          : 7875A8C1
2. 2b2s3230.ima with MD5 checksum      : 8FFAE4FC250E3ECA34C9E63C368BE3C3
3. 2b2s3230.ima_enc with MD5 checksum  : 2169B37C3EC2CAE363F10E81168E0D6E

[Added]:
S2BV       1. Supported OCP temperature.
S2BV       2. Supported 2U 3.5 EXP HSBP on S2BV.

[Changed]:
S2BX_S2SX  1. BMC will make sure there is no any NCSI transaction before it changed NCSI gpio pin.
S2SR       2. Updated the threshold value of P12V to 14.4 voltage if BBU is in dischaged mode.

[Bug Fixed]: N/A

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.22.00
=====================================================================
Version: 3.22.00
Release Date: 2014.12.05

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.09.02)

[Firmware Images]:
1. 2b2s3220.ima with checksum          : 7880B6AA
2. 2b2s3220.ima with MD5 checksum      : 058B42EBC7A1230188F4FD91BF0F6CD1
3. 2b2s3220.ima_enc with MD5 checksum  : 553CFE5E10CB7F75FE0586A179C342EA

[Added]: N/A

[Changed]:
S2BX_S2SX  1. Improved NCSI handling.
S2SR       2. Changed to monitor BBU sensors when system is in DC-on only.

[Bug Fixed]:
S2SR:
     154345 - BMC would report \A1\A7Battery_PSU_STA-Predictive Failure -Asserted\A1\A8 event when BBU capacity reach to 100% then unplug power cable.
     154333 - Node1 BMC Dashboard still show BBU sensor(temp, capacity, input and output) while node1 was power off and node2 was power on.
	 154331 - Node 2 BMC sensor couldn\A1\A6t record HDD0~HDD11 Driver slot(Bay) logs after BBU in discharge mode with turn off front HDDs.
	 154325 - The BMC SEL would record this \A1\A7Volt P12\A1\A8log when BBU discharge mode to 0% and system to do forced shutdown.
S2BP:
     153603 - BMC IP Address in BIOS Setup would not change immediately for the first time boot after set ''BMC LAN port configuration'' to ''Share-NIC (OCP Mezz)'' and then save & reset.

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.21.00
=====================================================================
Version: 3.21.00
Release Date: 2014.11.27

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.09.02)

[Firmware Images]:
1. 2b2s3210.ima with checksum          : 787F8C7C
2. 2b2s3210.ima with MD5 checksum      : 1E6CDA587416EF87697E8D8C8CC49FC0
3. 2b2s3210.ima_enc with MD5 checksum  : 1E0025E16BDD0F33FE2227D4D78F216F

[Added]:
S2BX_S2SX  1. Synchronized RTC time once BMC received "POST END" command.
S2SR       2. Added BBU firmware version in WEBUI dashboard.
S2BV       3. Supported TESLA K80 GPGPU.

[Changed]:
S2BP_S2SP  1. Removed the fault LED feature for Samsung PCISSD.
S2SR       2. Changed BBU device.
S2BP       3. Updated threshold value for NVMe_SSD sensor.

[Bug Fixed]:
S2BP:
     154106 - The PSU information are not displayed in BMC Dashboard.
     153603 - BMC IP Address in BIOS Setup would not change immediately for the first time boot after set ''BMC LAN port configuration'' to ''Share-NIC (OCP Mezz)'' and then save & reset.
	 153685 - Event ''OEM Record c0'' cannot decode to correct sensor name in SNMP Trap.
	 153624 - Event ''OS Boot Completed- Asserted'' cannot decode to correct sensor name in SNMP Trap.
     153596	- Event ''PEF Action - Asserted'' Severity is ''Information'', but it would cause Status LED be ''Amber Blinking''.
	 153496 - The Temp_SSDx will disappear when the SUT is DC off, and it will appear when SUT DC on.
S2BV:
     153682 - WebUI will display TESLA K80 VGA card device sensor with "N/A".
S2SP:
     151589 - The PCIe SSD Temperature sensor name is ''Temp_SSD0, Temp_SSD1'' It will confuse users.

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.20.00
=====================================================================
Version: 3.20.00
Release Date: 2014.11.17

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.09.02)

[WARNING]:
1. Please be noted that BMC FW 3.17 has been updated configuration files.
and please don't preserve the configuration settings if you want to upgrade/downgrade BMC firmware between firmware 3.17 or above and firmware 3.16 or below.

[Firmware Images]:
1. 2b2s3200.ima with checksum          : 7889BFE8
2. 2b2s3200.ima with MD5 checksum      : 3FE57D380430B4CB8276CDE8E61AD17F
3. 2b2s3200.ima_enc with MD5 checksum  : 7F0C48C803F58A326B22FF0A56795E3E

[Added]:
S2SR       1. Add BBU shutdown event log.
S2SR       2. Support "Clear fault" to clear BBU device.

[Changed]:
S2BP_S2SP  1. Changed PCIeSSD temperature name to "NVMeSSD_X".

[Bug Fixed]:
S2SR:
     152948 - [DVT2-ALL] The BMC would record this''volt P12V''log when battery capacity is lower than 40% ,and then insert power cord into chassis.
	 152925 - [DVT2-All]Couldn't verify OCP/OTP/OVP function of BBU due to BBU limitation. SIT doesn't know the function and SEL is workable or not.
S2SP:
     151589 - The PCIe SSD Temperature sensor name is ''Temp_SSD0, Temp_SSD1'' It will confuse users.

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.19.00
=====================================================================
Version: 3.19.00
Release Date: 2014.11.10

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.09.02)

[WARNING]:
1. Please be noted that BMC FW 3.17 has been updated configuration files.
and please don't preserve the configuration settings if you want to upgrade/downgrade BMC firmware between firmware 3.17 or above and firmware 3.16 or below.

[Firmware Images]:
1. 2b2s3190.ima with checksum          : 788815CF
2. 2b2s3190.ima with MD5 checksum      : 2BA378E1A483EF781A042181B397A5C8
3. 2b2s3190.ima_enc with MD5 checksum  : EE094EB06077141720FA0EE2A3A9A4E4

[Added]:
S2BP_S2SP     1. Support the fault LED feature for Samsung PCISSD.
S2SR          2. Support BBU status/state sensor.

[Changed]:
S2BP          1. Update fan table for SKU1. 
S2SR          2. Update the threshold value for BBU temperature.

[Bug Fixed]:
S2SR:
     152861 - [DVT2-2.5] Sometime system reports Battery low -Asserted/Deasserted log during run DC cycles test.
	 153029 - [DVT2-ALL]The battery input value doesn't match with BBU spec defined during BBU charge mode.

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.18.00
=====================================================================
Version: 3.18.00
Release Date: 2014.11.03

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.09.02)

[WARNING]:
1. Please be noted that BMC FW 3.17 has been updated configuration files.
and please don't preserve the configuration settings if you want to upgrade/downgrade BMC firmware between firmware 3.17 or above and firmware 3.16 or below.

[Firmware Images]:
1. 2b2s3180.ima with checksum          : 78840FE9
2. 2b2s3180.ima with MD5 checksum      : 900EC9578BAB11D6EE0856CF77875ECF
3. 2b2s3180.ima_enc with MD5 checksum  : E5A91A1A0821AE7B27DB64AFC7CC1929

[Added]:
S2SR          1. Supported OEM commands for upper layer tool to control S2SR system.
S2SR          2. Supported battery low event log for BBU.
S2SP          3. Supported PCIE SSD LED control.
S2BV          4. Supported K40/K8/K80 GPGPU devices.

[Changed]:
S2BX_S2SX     1. BMC used two data bytes to receive temperature data if thermal sensor is LM75 or TMP75 series.
S2SR          2. Updated threshold value for expander temperature.
S2SR          3. the upper critical threshold changed to 13.14v if the BBU device is in discharge mode.
S2SR          4. 1U CPU supported 40 degree MB thermal trip. 2U CPU supported 35 degree MB thermal trip.
S2BV          5. the fan speed will running to max. duty if any one GPGPU card not present.

[Bug Fixed]:
S2SR:
     152195 - [DVT2-All] Idle system few minutes BMC would log ''Temp_Exp_CPU Upper Non-Critial Going High -Asserted'' event on node1.

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2BV/S2BP/S2SR/S2SP AST2400 BMC FW Release v3.17.00
=====================================================================
Version: 3.17.00
Release Date: 2014.10.17

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]:
1. SOCFLASH (version v.1.09.02)

[WARNING]:
1. Please be noted that BMC FW 3.17 has been updated configuration files.
and please don't preserve the configuration settings if you want to upgrade/downgrade BMC firmware between firmware 3.17 or above and firmware 3.16 or below.

[Firmware Images]:
1. 2b2s3170.ima with checksum          : 7891EF1E
2. 2b2s3170.ima with MD5 checksum      : C3BC9E9263A9624200E52380CFD5F3E7
3. 2b2s3170.ima_enc with MD5 checksum  : 844A009A727146A925F463B2FC9CE521

[Change/Add]:
S2BX_S2SX 1. Changed the script privilege of WEBUI service before rsync service.
S2BX_S2SX 2. Improved the I2C driver in u-boot code.
S2BV          3. Support GPGPU devices on different i2c bus.
S2BV          4. Update Fan table.
S2SR          5. Support BBU temperature and BBU PSU status sensors.
S2SR          6. Update PTAS C value.

[Bug Fixed]:
S2SR:
     152015 - [DVT2-All] Please define the OCP/OVP/OTP behavior of BBU on BMC WEBUI.
	 152010 - [DVT2-All] BMC WEBUI not display BBU temperature sensor ,but BBU SPEC Rev:0D have defined.
	 151438 - [DVT2-All] BMC chipset revision was show ''AST2300'' in BMC FW release note.(should be AST2400)
	 151090 - [DVT2-All]MB position was incorrect (node1 show 2, node2 show 4) in BMC WebUI.
S2BV:
	 151387 - SEL has ''Upper Non-Critical - Going High'' event logs during stressing NVIDIA K20X in win2012r2.
	 151145 - WebUI does display nVidia GPGPU Card device sensor N/A. 

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=XXXX.ima -s option=x flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2B/S2BP/S2S/S2X AST2300/AST2400 BMC FW Release v3.16.00
=====================================================================
Version: 3.16.00
Release Date: 2014.09.25

AMI Subversion Revision: AMI SPX 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3160.ima with checksum          : 78F8A49F
2. 2b2s3160.ima with MD5 checksum      : D2C2D00D23C9625E59A0F33DFCBFBF7F
3. 2b2s3160.ima_enc with MD5 checksum  : 3044087D640FA8D72EF4172B226A6C75

[Change/Add]
S2B_S2BX_S2S_S2SX  1. Follow IPMI Spec. 2.0 rule to access BIOS version string if the string is over 14 bytes.
S2B_S2BX_S2S_S2SX  2. Improve the error handling on PEF postpone timer task.
S2B_S2BX_S2S_S2SX  3. Support "Get Server Node Health status" command for QDCM.
S2B_S2BX_S2S_S2SX  4. Change watchdog timer value in ASPEED chipset. Runtime is 15 seconds. BMC update mode is 900 seconds.
S2S_S2SP           5. Support the temperature sensor for OCP X540.
S2SP_S2BP          6. Support the temperature sensor for Samsung PCIESSD.
S2BP               7. Support the temperature sensor for QCT Mezz card.
S2BP               8. Update fan table and PTAS C value for SKU0/1/2.
S2SR               9. Update HDD status to X5M depended on motherboard position.
S2SR              10. Change command code ID for remote bios update (RBU).

[Bug Fixed]
S2B:
	150873 - BMC HDD Sensor detection for S2B 3.5'' 1-1 SKU is not matched the physical connection in BP.
	150389 - After DC off, BMC still have Airflow reading in Dashboard.
S2BP:
	150688 - WebUI Temp_SSDx Value is shown "NA" with Samsung PCIe SSD.(PCIe SSD : (Samsung)MZWEI400HAGM-00003 SSD,PCI-e,400GB).
	150398 - After boot into W2012R2, the pie chart will display ''Memory Event'' in Event Logs list but the event is OS Boot .
	150252 - The PCIE Error / POST Error / QPI Error / Memory Error sensor number are all 00h, they are mismatched with BMC Spec defined.
S2S:
	149907 - SUT get BMC time and version check fail during warm boot cycling.
S2SP:
	150728 - After flash BIOS S2SP2A03, the BMC WebUI can\A1\A6t show correct BIOS version.
SMS01:
	150617 - [S2B] It's can't display current system ''HEALTH STATUS'', S2RQ works normally.

[Known issue]: N/A

[Notice]:
	1. Update BMC FW via command line:
		a) put dos4gw.exe, socflash.exe, and rom.ima in same directory.
		b) in DOS, run "dos.bat".
		   in Window, run "win.bat"
		   in Linux, run "linux.sh"
	2. Force to update BMC FW via command line:
		a) run "socflash if=rom.ima cs=0 flashtype=2" in DOS.
	3. Update BMC FW via Web UI:
		a) Please select rom.ima_enc as image file and doesn't upload Signimage key.
	4. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: admin

=====================================================================
        S2B/S2BP/S2S/S2X AST2300 BMC FW Release v3.15.00
=====================================================================
Version: 3.15.00
Release Date: 2014.08.28

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3150.ima with checksum          : 7C181CF6
2. 2b2s3150.ima with MD5 checksum      : 81EDE28A9BB25BAF24BF714C834653BE
3. 2b2s3150.ima_enc with MD5 checksum  : F3C213B5B6EABA04C9FF202BA260EAA9

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2BX_S2S_S2SX 1. Support BIOS firmware update through Yafuflash tool.
S2B_S2BX_S2S_S2SX 2. Support BIOS version string to 28 bytes.
S2S_S2SX          3. X5M is unable to get repeater table if user pressed power button after IPMI stack is ready but it not handshaking with X5M yet.
S2BV              4. Add GPGPU temperature sensor.

[Bug Fixed]:
S2SR:
149753 - [DVT-All]BMC WebUI can\A1\A6t show BIOS complete name.

S2SP:
149842 - The BMC WebUI can\A1\A6t show BIOS complete name(S2SR Issue ID 149753)
149741 - After flash BMC to 31.14, the WebUI cannot show correct BIOS version when system in BIOS POST(After POST End can show correct BIOS version)

[Known issue]: N/A

=====================================================================
        S2B/S2BP/S2S/S2X AST2300 BMC FW Release v3.14.00
=====================================================================
Version: 3.14.00
Release Date: 2014.08.14

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3140.ima with checksum          : 7DB89601
2. 2b2s3140.ima with MD5 checksum      : 1EC2609E2194208D3FFDE9A5CD2521B6
3. 2b2s3140.ima_enc with MD5 checksum  : A8926DCBE9FB53D6FD549431D96A27B8

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2BP_S2S_S2SX 1. Change the field of DIMM size to 4 bytes in OEM Set/Get DIMM information.
S2B_S2BP_S2S_S2SX 2. Improve NCSI fail-over function.
S2B_S2BP_S2S_S2SX 3. Support single sign on support Web UI & KVM.
S2BP              4. Add PCI SSD temperature.
S2BP              5. Update fan table.

[Bug Fixed]:
S2S:
149188 - [BIOS Final Reg](3A12)When change the RAS mode to Lockstep Mode, BMC WebUI displays all wrong memory size as 0 MB(memory size detects correctly in BIOS ).
149090 - [BIOS Final Reg][Reg-5]The BMC SEL is unable to list all event logs after just inject Memory Un-Correctable Error and next boot.
148848 - [Issue SYNC ]The BMC shared-NIC doesn't work with OCP Mezz card(i350),(S2SR 148044)

S2SR:
148044 - [DVT-All]The BMC shared-NIC doesn't work with OCP Mezz card(10Gb 82599,i350)

S2BP:
149176 - The Volt_P3V_BAT is mismatched the BMC FW spec defined.
149289 - The BMC Shared-NIC Fail-over function is not work.
149020 - Fan duty is abnormal when systems stress at 25C and 0C.
148475 - WebUI display current DIMM channel number do not match with DIMM slot of M/B.

[Known issue]: N/A

=====================================================================
        S2B/S2S/S2X AST2300 BMC FW Release v3.13.00
=====================================================================
Version: 3.13.00
Release Date: 2014.07.29

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3130.ima with checksum          : 7F4E0C03
2. 2b2s3130.ima with MD5 checksum      : 7B2444FD63294278BD70459494F7C484
3. 2b2s3130.ima_enc with MD5 checksum  : AB02FB20B25222E99FED43CBCA84DC7A

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S_S2SX 1. Change memory error/QPI/POST error/PCIE error/memory event sensors to event only.
S2S_S2SX     2. Remove HDD FRU for X5M.
S2S_S2SX     3. Support repeater table version 3 for X5M system.
S2SR         4. Improve remote bios update through BMC video memory space (RBU).
S2B          5. Issue "Clear PSU fault" command if AC lost flag of PSU is been triggered.
S2B          6. Support UV fault and UV warning detection for PSU.

[Bug Fixed]:
S2S:
148414 - SEL ''PSU1 Status | Power Supply Input Lost (AC/DC)-Asserted'' recorded randomly during AC cycling test.

S2SR:
148164 - [DVT-All]The BP-FRU info has garbage string in BMC WebUi.
148083 - [DVT-All]BMC SEL will record "Power Supply Input Lost(AC/DC-Asserted) of ''PSU1 status'' during manual AC on/off testing.
148044 - [DVT-All]The BMC shared-NIC doesn't work with OCP Mezz card(10Gb 82599,i350).
148030 - [DVT-All]BMC log \A1\A7Drive Presence\A1\A8 HDD9 doesn\A1\A6t meet the sequence while system power on.

S2B:
148407 - (DELTA DPS-500AB-14) Run AC cycling with only 1 power cord inserted on PSU2 and it will log Power Unit Failure detected.

[Known issue]: N/A

=====================================================================
        S2B/S2S/S2X AST2300 BMC FW Release v3.12.00
=====================================================================
Version: 3.12.00
Release Date: 2014.07.14

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3120.ima with checksum          : 7F588C23
2. 2b2s3120.ima with MD5 checksum      : D34107DBF2F1092D0792B17DE58AEE38
3. 2b2s3120.ima_enc with MD5 checksum  : 34E7E969C72C132867F35F1D2A2807F7

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B       1. Update fan table for SKU3/4/5.
S2SR      2. Support remote bios update through BMC video memory space (RBU).
S2SR      3. Support backup battery unit (BBU).

[Bug Fixed]:
S2B       1. PSU configuration is unable to restore to default through WEBUI.
S2S_S2SX  2. Fixed no sensor reading on PSU 2 Status / PSU redundant reading sensors.

S2SR:
147974 - [DVT-All]Get the Temp_SSDx reading are show all ''N/A''on BMC WebUI.
147851 - [DVT-3.5]The sensor reading value of sensor''HDDx'', should be shown HDD0~11 on BMC WebUI when insert HDD 12 pcs on 3.5 chassis.

[Known issue]: N/A

=====================================================================
        S2B/S2S/S2X AST2300 BMC FW Release v3.11.00
=====================================================================
Version: 3.11.00
Release Date: 2014.06.30

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3110.ima with checksum          : 80E68382
2. 2b2s3110.ima with MD5 checksum      : C006CB7C31D1016ABCBFD44393DCE4BC
3. 2b2s3110.ima_enc with MD5 checksum  : F7CA252271C02D3E22EC1BB8FA75810A

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S_S2SX 1. Add Intel QDCM OEM commands.
S2B_S2S_S2SX 2. Support NCSI fail-over function.
S2B          3. Support the cold redundant settings in WEBUI. (WEBUI->Confiugration->Power supply).
S2B          4. Support one power supply or two power supplies settings in WEBUI. (WEBUI->Confiugration->Power supply).
S2B_S2S_S2SX 5. Change AC drop behavior. 

[Bug Fixed]: N/A

[Known issue]: N/A

=====================================================================
        S2B/S2S/S2X AST2300 BMC FW Release v3.10.00
=====================================================================
Version: 3.10.00
Release Date: 2014.06.19

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3100.ima with checksum          : 8103ECBD
2. 2b2s3100.ima with MD5 checksum      : B6FB0ABC45B1948ECCB3F72C3FB8594A
3. 2b2s3100.ima_enc with MD5 checksum  : 5B856207939A32214B0F0FF153681133

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2SP 1. Update PCIE SSD temperature to X5M FW through sensor exchange command.
S2B  2. Spport HVDC PSU.

[Bug Fixed]: N/A

[Known issue]: N/A

=====================================================================
        S2B/S2S/S2X AST2300 BMC FW Release v3.09.00
=====================================================================
Version: 3.09.00
Release Date: 2014.06.16

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3090.ima with checksum          : 81011093
2. 2b2s3090.ima with MD5 checksum      : A7127BDC90C88BD6457EDC4B90A183B1
3. 2b2s3090.ima_enc with MD5 checksum  : 95F9CED5C8961B3EF3D7218B657C9886

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S_S2SX 1. Change "PSU Status" sensor behavior from only DC OFF monitor to DC ON/OFF monitor.

[Bug Fixed]:
S2B:
147267 - After Clear FP FRU and make AC cycle, tha System Fan will not working after power on.
147233 - Event severity is Unspecified after Other IIO error injected in SEL.
147232 - Sensor Name is showed as ''Airflow'' for Other IIO error log in SEL.
147229 - ''OEM Record c0'' displayed incorrect sensor name and description in SNMP Trap / PEF mail log.
147219 - BMC will read Fan speed to 20000 rpm if set the fan duty lower than 10 (0Ah).
147217 - WebUI will not work after SNMP trap is enabled and do a system reboot cycle.
147098 - [SDA]BMC sometimes got PCIE SSD1 FAN 0 rpm reading.

S2S:
147142 - There is no definition and no log recorded after system auto power off caused by PSU fault.

[Known issue]: N/A

=====================================================================
        S2B/S2S/S2X AST2300 BMC FW Release v3.08.00
=====================================================================
Version: 3.08.00
Release Date: 2014.06.05

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3080.ima with checksum          : 8108F629
2. 2b2s3080.ima with MD5 checksum      : 6A8DA724C2BADDA91838C8953770A823
3. 2b2s3080.ima_enc with MD5 checksum  : AD884DF565A411E595CED1EFA0346D0C

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S_S2SX 1. Added the compensating sensing method for AST2400 ADC module.
S2B          2. Fixed to return the wrong Fan RPM reading to ME FW.

[Bug Fixed]: N/A

[Known issue]: N/A

=====================================================================
        S2B/S2S/S2X AST2300 BMC FW Release v3.07.00
=====================================================================
Version: 3.07.00
Release Date: 2014.05.29

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3070.ima with checksum          : 81050B95
2. 2b2s3070.ima with MD5 checksum      : 4789C591B67B3032392EF71083B4BB86
3. 2b2s3070.ima_enc with MD5 checksum  : 391F769757236F595401BC8D30F47623

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S_S2SX 1. Update the threshold value and retry 3 times for 1.05v sensor.
S2B_S2S_S2SX 2. Update the worst card table for smart fan control.
S2B_S2S_S2SX 3. Improve to update the thermal coefficient value based on HDD quality.
S2S_S2SX     4. Disable GPIO pass-through feature for power button and NMI button.

[Bug Fixed]:
S2S:
146717 - BMC hasn't finished initiation yet (heartbeat LED is dark), SUT 80 port LED and HDD LED started to flash/scan as soon as MB insert chassis then press power button.
146353 - [AST2400]Remote connect SUT screen by BMC RKVM, change the resolution 1440 x 900,1600 x 900,1680 x 1050 under W2K12R2, the screen would shake.(F06A ID:145990)

[Known issue]: N/A

=====================================================================
        S2B/S2S/S2X AST2300 BMC FW Release v3.06.00
=====================================================================
Version: 3.06.00
Release Date: 2014.05.22

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3060.ima with checksum          : 810412D5
2. 2b2s3060.ima with MD5 checksum      : F1B1498A0016C2ECFD7A444256F0C036
3. 2b2s3060.ima_enc with MD5 checksum  : C4BB13D1FE31A30FB1492EB949653490

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S_S2SX 1. Add DHCP retry mechanism for some OCP cards not support AEN.
S2B_S2S_S2SX 2. Add a mechanism to clear the invalid system MAC address.
S2B_S2S      3. Support dynamic thermal coefficient value based on HDD quality.

[Bug Fixed]:
S2B:
146315 - [Single board issue] WebUI System MAC will show 2 onboard LAN1 address.

S2S:
146717 - BMC hasn't finished initiation yet (heartbeat LED is dark), SUT 80 port LED and HDD LED started to flash/scan as soon as MB insert chassis then press power button.
146541 - [BIOS Final Reg] Abnormal ''Power difference'' log recorded during SUT AC cycling test.
141424 - FSC SPEC (Temp_Outlet) is under definition (calculated by Intel PTAS) , plan to be ready by DVT2.

[Known issue]: N/A

=====================================================================
        S2B/S2S/S2X AST2300 BMC FW Release v3.05.00
=====================================================================
Version: 3.05.00
Release Date: 2014.05.08

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3050.ima with checksum          : 80258C6B
2. 2b2s3050.ima with MD5 checksum      : 373B9FB67ED57A2F7F21DFE964BB6924
3. 2b2s3050.ima_enc with MD5 checksum  : D1CA5DE180204E00FCD65B8E8C0E49EF

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2S  1. Add EQ setting in repeater data structure.
S2S  2. Load the different coeficient value based on different HDD configuration.
S2SX 3. Add SSD temperature sensor.

[Bug Fixed]: N/A

[Known issue]: N/A

=====================================================================
        S2B/S2S AST2300 BMC FW Release v3.04.00
=====================================================================
Version: 3.04.00
Release Date: 2014.04.29

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3040.ima with checksum          : 802DC22B
2. 2b2s3040.ima with MD5 checksum      : 484679C10FDCB61BD6EB4D28E9EBC51C
3. 2b2s3040.ima_enc with MD5 checksum  : DD5901573C9E746B2651417B7395F6A3

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S 1. Added OEM command to enable or disable "Keep PHY link UP" feature. (Enabled:\A1@ipmitool raw 0x30 0x91 0x5a 0x00 0x00 0x01\A1@/\A1@Disabled: ipmitool  raw 0x30 0x91 0x5a 0x00 0x00 0x00)
S2B_S2S 2. Enable GPIO pass-through feature for power button and NMI button.

[Bug Fixed]:
S2B:
146105 - BMC port link LED will blinking amber when it's connected 1G LAN.
146091 - Use a stick to stop PSU fan, the PSU LED will change to Amber but BMC will not log power Supply Failure Detected.
145923 - [SmartFSC] Some worst Card will not have correct Weighted as design.
145913 - Severity of ''OEM Record c0'' is showed as ''Information'', but defined as ''Critical'' in ''QCI_SPX_EventLogTable_v1.15''.
145817 - Severity of event ''Software NMI - Asserted'' is not correct that showed as ''Warning''.
145719 - If not install the DIMM in channel A,B / G,H, BMC will get the channel reading as 0, not NA.

S2S:
145712 - OCP I350 connection ping lost during SUT warmboot when use I350 as BMC shared-NIC.

[Known issue]: N/A

=====================================================================
        S2B/S2S AST2300 BMC FW Release v3.03.00
=====================================================================
Version: 3.03.00
Release Date: 2014.04.16

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3030.ima with checksum          : 8030441F
2. 2b2s3030.ima with MD5 checksum      : AE9C550625683DF626AC90E0EC9E2F96
3. 2b2s3030.ima_enc with MD5 checksum  : 6BF158ECFA04DB7017C9E755AE4F4DA5

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S 1. Updated the new PCIE special cards table and please refer to support list at the end of file.
S2B_S2S 2. Added to detect chipset is AST2300 or AST2400.
S2B     3. Update the parameters of smart fan control.
S2B     4. Disable the event log of "system NIC link" sensors.

[Bug Fixed]:
S2B:
145524 - The DIMM Temperature will display NA if only insert the DIMM on A0, B0, C0, D0, E0, F0, G0, H0.
145540 - [AST2400 M/B] The BMC Chipset of device information should display AST2400 if the BMC chip is AST2400 (display AST2300)
144789 - WebUI/Dashboard didn't show Onboard LAN MAC Address.

S2S:
144839 - [PVT]Insert one DIMM per channel in the system , the Temp sensor status will show NA on BMC WebUi.(Two DIMM per channel Temp status is OK.)
145254 - [PVT]Use two different PMBus version PSUs and insert into chassis,the system doesn't log the event ''PSU - PSUx - PMBUS Version mismatch. - Asserted'' on BMC WebUi.
145512 - [PVT][AST2400]The BMC Chipset show AST2300 on BMC WebUi.(Should show AST2400 chipset)
145562 - [PVT][AST2400]The event sensor name description: ''Linking Board status error - Asserted'' and ''Programming HDD repeater failed - Asserted'' would show [undefined Sensor Specific event] on remote email alert.
145067 - [PVT]After update BIOS FW 3A02 via BMC WebUi,the system will log ''SPS FW Health-Firmware status-Internal Error/Firmware Exception - Asserted on BMC WebUI.

[Known issue]: N/A

=====================================================================
        S2B/S2S AST2300 BMC FW Release v3.02.00
=====================================================================
Version: 3.02.00
Release Date: 2014.04.03

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3020.ima with checksum          : 803AC884
2. 2b2s3020.ima with MD5 checksum      : 288423F4ADEBD035D620E16C75F46592
3. 2b2s3020.ima_enc with MD5 checksum  : 7AE2BEC532388E6824290346F42D3EF3

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S 1. Add OEM command to enable or disable VR monitoring. (ipmitool raw 0x30 0xd2 0x1/ipmitool raw 0x30 0xd2 0x1)
S2B_S2S 2. Add AER enabled for AST2400.
S2B_S2S 3. Update the sensor conditions for fault LED control.
S2B     4. Changed sensor name from "Fan_Card"/"Temp_PCIE_SSD" to "Fan_SSD"/"Temp_SSD".
S2B     5. Add OEM sensor to detect Power difference.
S2S     6. Add OEM sensor to detect PMBus version mismatch.
S2S     7. Update the threshold value for ambient sensor.

[Bug Fixed]:
S2S:
145254 - [PVT]Use two different PMBus version PSUs and insert into chassis,the system doesn't log the event ''PSU - PSUx - PMBUS Version mismatch. - Asserted'' on BMC WebUi.
145218 - WebUI(Server Hearth/Filtered by: ) should list all disk number (HDD0 to HDD23) since the max supported disks for 2.5/3.5 is 6/3 only.
144909 - [PVT]After system occur the event ''Rebuild/Remap in progress - Asserted'' (Severity:critical) on BMC WebUi,the Power Button LED on X5M front panel will not amber blinking.
144772 - HDD BMC log description: ''Drive Presence'' was fail to show up on remote email alert.

[Known issue]: N/A

=====================================================================
        S2B/S2S AST2300 BMC FW Release v3.01.00
=====================================================================
Version: 3.01.00
Release Date: 2014.03.28

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3010.ima with checksum      : 804083D4
2. 2b2s3010.ima with MD5 checksum  : 04D1C790768B7B98DB7E31F4DD9AEE56

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S 1. Fix the compatible issue with the grid table on IE and Chrome.
S2B_S2S 2. Support to get CPLD UES ID. (ipmitool raw 0x30 0x17 0x3)
S2B_S2S 3. Enable BMC HW watchdog feature.
S2B_S2S 4. Changed BMC FW info sensor to log "PSU mis-match" and "power difference event" logs.
S2B_S2S 5. Follow thermal rule to support graceful shutdown the system.
S2B_S2S 6. Fix BMC will response the incorrect power consumption to ME.
S2B_S2S 7. Support remote BIOS configuration specification v0.6.
S2B_S2S 8. "PSU alert" sensor only monitor on system DC on.
S2B     9. Change the behavior from Interrupt mode to Polling mode for "system NIC link" sensor.
S2B     10. If any fan speed in zone is lower than 500 rpm, the fans of this zone will set to 100 fan duty for 1U chassis. 95 fan duty is for 2U chassis.  
S2B     11. Fix BMC will not log "Drive fault" event log.
S2B     12. Update the threshold value for fan and ambient sensors.
S2B     13. Update fan table for SKU4 and SKU5.
S2S     14. If system is DC off, BMC always return "PCIE card not present" to CMC.

[Bug Fixed]:
S2B:
145018 - Continued #144853. Event ''SYS_NIC1_LinkUp | LAN | Deasserted'' will be recorded after reboot cycle.
144928 - [2U 2.5'' Expander] SEL doesn't have ''Drive Fault'' events when RAID is degarde in win2012r2.
144665 - New Feature for get CPLD Version via IPMI command is not ready.
142992 - [Predictive Power Cap] The power consumption will not approach the limit power consumption of the power policy set.

S2S:
145047 - [PVT] The Sensor name(PSU Alert) couldn't show correctly (it showed: 0x6d) on SEL list by using IPMI command(IPMItool ver.1.8.13)

[Known issue]: N/A

=====================================================================
        S2B/S2S AST2300 BMC FW Release v3.00.00
=====================================================================
Version: 3.00.00
Release Date: 2014.03.20

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s3000.ima with checksum  0x803AC924

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S 1. Support the new Set/Get MAC Address command.
S2B     2. Update FAN control table for SKU 3 and SKU4.
S2B     3. Add new sensors for two system NIC status.
S2B     4. Update the threshold value for Temp_Ambient/Temp_PCI_Inlet1/Temp_PCI_Inlet2 sensors.
S2S     5. Clear HSC fault flag once when system was DC on.

[Bug Fixed]:
S2B:
144312 - BMC Dedicated LAN Speed LED is always blinking.

S2S:
143129 - The SPEC about Shared-NIC options on BMC WebUI for different LAN devices hasn!|t been confirmed yet.

[Known issue]: N/A

=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.17.00
=====================================================================
Version: 2.17.00
Release Date: 2014.03.13

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s2170.ima with checksum  0x805225B2

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S 1. BMC will trigger CPLD to restore system power status if system power dropped.
S2B     2. Added the new PCIE special cards in BMC and please refer to support list at the end of file.
S2B     3. Update FAN control table.

[Bug Fixed]:
S2B:
143897 - 'Current BMC LAN Port State' is not changed after set 'BMC LAN Port Configuration' to 'OCP Mezz' or 'Quanta Mezz'.
143764 - BMC WebUI get the Temp_PCIE_SSD and Fan_CARD reading are all NA.

S2S:
144116 - BMC got unexpected log ''PSU Alert, State Asserted - Deasserted'' during CMC FW flash overnight.
144211 - The ReleaseNote doesn't provide ''Bug Fixed'' list in BMC Fw 2.16 package.
143624 - BMC recorded log ''HW watchdog timeout reset'' almost 16mins after idle in web FW flash mode.(should be 18mins later and record another log).
144068 - After run DC on/off stress under Ubuntu 12.04.03 127cycles(10hrs), BMC will occurred some abnormal SEL. one of sled occurred ''Power Unit Failure Detected - Asserted''.

[Known issue]: N/A

=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.16.00
=====================================================================
Version: 2.16.00
Release Date: 2014.03.06

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s2160.ima with checksum  0x8090F0BA

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Change]:
S2B_S2S 1. Update sensor reading fuction for SNMP.
S2B_S2S 2. Added to support Shared NIC selection.
S2B_S2S 3. Changed SOL baudrate to 115200.
S2B_S2S 4. Update DCMI configuration.
S2B_S2S 5. Added PCIE card information to FSC PID and CMC.
S2B_S2S 6. Fixed SOL sending error.
S2B     7. Not show PCIE SSD tempeature and FAN card sensors in WEBUI if the device is not present.
S2S     8. Not handle CATERR signal after system is power on in 5 seconds.

[Bug Fixed]:
S2B:
142847 - SEL has '' PSU Predictive Failure - Asserted'' warning logs when SUT is idle or one PSU AC on/off.
142111 - System recorded abnormal event ''BMC FW info - PSU - PSU2 - Version mismatch. - Asserted'' in SEL
143930 - After change the RKVM mouse mode to ''Other Mode'' then the RKVM cannot zoom in or zoom out.
143863 - BMC Web UI SOL Baud Rate default setting is mismatched with BMC design Standardization v019 and ESMS Spec v054
143831 - ''Current BMC LAN Port State'' will become ''Share-NIC (LOM)'' after update BIOS to 2A14. But function is work on Dedicated-NIC.

S2S:
143860 - One of sled occurred CPU CATERR ''Uncorrectable Error'', when execute DC on/off stress under Ubuntu 12.04.03 about 110cycles (11hrs)
143768 - After run DC cycles for 24hrs (178 cycles) , the BMC LAN Port state would change automatically from ''Dedicated-NIC'' to ''Shared-NIC'' in BIOS setup
143552 - There have some sensor number doesn't define in S2S BMC Temperature Monitor table on MibBrowser tool.
143383 - The temperatureStatusOverall item will show ''unknown'' on MibBrowser tool when temperature senser status get normal value on BMC WebUi.
143775 - When BIOS BMC network shows ''Shared-NIC(LOM)'' but it's still linkable when connecting to Dedicated port.

[Known issue]:
        1. Smart Fan only support a PEIC card so far, the card model: vendor ID:0x1000/device ID:0x97/subvendorID:0x152d/subdeviceID:0x0

=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.15.00
=====================================================================
Version: 2.15.00
Release Date: 2014.2.27

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s2150.ima with checksum  0x7B73AA9A

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2B_2S] 1. Add new sensor "Temp_PCIE_SSD0", "Temp_PCIE_SSD1","Fan_CARD0",Fan_CARD1". for sku1,2,4,5.

[Change/modify/Remove]
[S2B_S2S]1. modify the threshold of VRHOT_EVENT_TEMP_THRESHOLD to 75 from 90.
[S2B_S2S]2. (142774)(Raincer)fix BIOS Post Error Undefined event.
[S2B_S2S]3. (143624)disable the watchdog of BMC.
[S2B]4. (142111,143642,143661)modify the MACRO "PEC VALIDATE" of PSU to 0.
[S2B]5. need update to EE from file if sku is mismatch.
[S2B]6. (143644,143595,143586,143595,143586)extend fan zone to zone5 for ME PTAS.
[S2S]7. (143707) add the code to send CPU offset to CMC.
[S2S]8. (143572)deal with PSU event when PSU present.

[Bug Fixed]:
143644 S2B Airflow, Temp_outlet, PSU input sensors are all displayed NA in Sensor Reading page. [Same as S2S : 143595,143586] 
142111 S2B System recorded abnormal event ''BMC FW info - PSU - PSU2 - Version mismatch. - Asserted'' in SEL.
143642 S2B The PSU Firmware version and MFR version are both NA in Web UI Dashboard.
143661 S2B BMC 2.14 will not log about AC input lost / Redundant Lost when remove the Power Cord. (Similar S2S 143572)
143595 S2S [DVT2]The Airflow sensor status and Current Reading will show ''NA'' on BMC WebUi.(2.14 failed; 2.13 passed)
143586 S2S [DVT2]The Temp_outlet sensor status and Current Reading will show ''NA'' on BMC WebUi.(2.14 failed; 2.13 passed)
143572 S2S No related BMC log recorded when unplug power cord from PSU.
142774 S2S [DVT2][2.5!|]POST Err inj test (ex. clear Password/CMOS; information level log), BMC error log detail would show !?Error unknown!|. 
143624 S2S BMC recorded log ''HW watchdog timeout reset'' almost 16mins after idle in web FW flash mode.(should be 18mins later and record another log). 
143707 S2S S2S BMC 2.13 cannot support CPU offset function. 
[Known issue]:
n/a
=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.14.00
=====================================================================
Version: 2.14.00
Release Date: 2014.2.21

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s2140.ima with checksum  0x7B724D4C

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2B_2S] 1. add get/set PCIE card cmd.(cmd:0x70/0x71)

[Change/modify/Remove]
[S2B_S2S]1. change the power off of mb_thermal_trip temp to 47 from 45.
[S2B_S2S]2. (143112)change the sensor to TEMP_VR_CPU0,TEMP_VR_CPU1,TEMP_VR_DIMM0,TEMP_VR_DIMM1,TEMP_VR_DIMM2,TEMP_VR_DIMM3, and temp threshold to 90 for VRHOT alert.
[S2B_S2S]3. (142682)change the cpu sensor name to Temp_CPU0 and Temp_CPU1 for temp and CPU_0 and CPU_1.
[S2B_S2S]4. (Raincer)modify SMASM version from 2012 to 2014.
[S2B_S2S]5. (142774)(Raincer)fix BIOS Post Error Undefined event.
[S2B_S2S]6. initial eventdesc for WebUI.(Raincer)
[S2B_S2S]7. (Raincer) such as Clear Password or CMOS/NVRAM cleared.
[S2B_S2S]8. (Raincer)remove error IPv6 filter 0200::/3.
[S2B_S2S]9. (Raincer)FC00::/7 Unique-Local equivalent to IPv4 private address space.
[S2B_S2S]10. change the HDD polling time to BIOS "POST START" from "POST END".
[S2B_S2S]11. (143262)change the temp comparison formula to "SIGN" for "MB thermal trip" function.
[S2B_S2S]12. (143290)change to PRIV_USER for command get_SKU_data and get_PSU_data. 
[S2B_S2S]13. remove OEM command "GET_SYS_FAN".
[S2S]14. judge the first byte of PSU MFR_REVISION to show 2 byte or 3 bytes.
[S2S]15. change the inlet temp to "Temp_Amblient_FP" 0xf9 for PTAS.
[S2S]16. read the PSU data only when psu insert.
[S2S]17. (143063)report the FAN sensor reading to N/A when it is disabled. 
[S2S]18. Send HDD qty and PCIE card type to CMC.
[S2B]19. modify the fan speed to 95% when fan fail in that zone.(include PCIE card zone.)
[S2B]20. change the PID sensor num rule.(include fanctrlsrc and fannum)
[S2B]21. update PID fan table "pid_setup".
[S2B]22. add the new temp sensor and fan sensor and fanctrl by PID for SSD PCIE card. (sku1 to sku5)
[S2B]23. (142595)(142591)(142585)remove the code to modify the hdd slot num for MG9094.
[S2B]24. (142111) add the PEC check code for PSU communication.
[S2B]25. add the code to cahnge the fan speec when hdd qty and pcie card type change.

[Bug Fixed]:
143112 S2S [DVT2] Use rework MB to test CPU_VR_HOT / DIMM_VR_HOT sensor and heat the sensor on MB,the system doens't log any message on BMC WebUi.
143063 S2S [DVT2] The sled1,2 BMC will alert ''Fan_SYS_2_1...Fan_SYS_3_2 0 RPM low critical'' on BMC WebUI when Sled3,4 Power status was DC off
142682 S2S [SPEC] Sensor name for CPU temp is different among BMC_Std_SPEC, Mechanical_Std_SPEC and BMC FW SPEC.
143290 S2S Error message popped when login BMC Web with operator account then access ''Sensor Readings'' page.
143262 S2S [SDA]When Temp_Ambient_FP attach to negative temperature, System shutdown and SEL show MB Thermal Trip
142774 S2S [DVT2][2.5!|]POST Err inj test (ex. clear Password/CMOS; information level log), BMC error log detail would show !?Error unknown!|.
142595 S2B [2U 3.5" one to one]SEL doesn't record rebuild status logs when RAID is rebuilding with LSI 2208.(Similar S2B #142585).
142591 S2B [2U 3.5" one to one]SEL doesn't record logs when removing one HDD by RAID1 with LSI2108.
142585 S2B [2U 3.5" one to one]SEL doesn't record rebuild status logs when RAID is rebuilding with LSI 2108.
142111 S2B System recorded abnormal event ''BMC FW info - PSU - PSU2 - Version mismatch. - Asserted'' in SEL.

[Known issue]:
n/a
=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.13.00
=====================================================================
Version: 2.13.00
Release Date: 2014.1.28

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1. 2b2s2130.ima with checksum  0x7B75391E

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2S_S2B]
n/a 

[Change/modify/Remove]
[S2B_S2S]1. Change code about the hdd slot for MG9094.(142595,142591,142585)
[S2B_S2S]2. Change the mapping table from 1-based to 0-based for event "POST Error -DIMM initialization fail" and "DIMM configuration problem".(142555)
[S2B_S2S]3. Update DHCP IP when BMC LAN port is changed between Dedicated-NIC and Shared-NIC.(Keven)(142130)
[S2B_S2S]4. Updated DHCP information after network confiuration finish.(Keven)(142130)
[S2B_S2S]5. It will retry to get system power status, since PCH will return error code sometimes.(Keven)(142745,142612,142606)
[S2B_S2S]6. change the code of log project/chassis event error.(142620)
[S2B]7. change the version compare rule for PID table from ">=" to ">".
[S2S]8. change the fan order (sensor name) from 0.(142504)
[S2S]9. change the power reading source from HSC to PSU from PTAS.


[Bug Fixed]:
142620 S2B BMC will not log the SKU - Project - Unavailability and SKU-Chassis-Unavailability after update the FRU without project name/chassis type.
142595 S2B SEL doesn't record rebuild status logs when RAID is rebuilding with LSI 2208.(Similar S2B #142585).
142591 S2B SEL doesn't record logs when removing one HDD by RAID1 with LSI2108.
142585 S2B SEL doesn't record rebuild status logs when RAID is rebuilding with LSI 2108.
142555 S2B ''POST Error - DIMM initialization fail'' location reported in SEL is not followed M/B DIMM Silkscreen.
142504 S2S [T1] The number order definition of X5M chassis FAN btw. BMC WebUI SPEC & Mechanical SPEC is different
142130 S2S [DVT AVL](ON 82599) Itdoesn't get correct IP address when exchange BMC port config with two network section in DHCP server
142745 S2S BMC event ''Power Unit Failure Detected-Asserted/Deasserted'' recorded during SUT MB/PDB/BP FRU read/write stress test (similar to S2S 142606) 
142612 S2S [DVT2] Sometimes PSU will alert ''Power Supply Failure Detected - Asserted'' SEL on BMC WebUI, when run CPU or DIMM stress under WS2012R2.(similar S2S ID:142560)
142606 S2S [DVT2] MB plug /un-plug sometimes would occur !\A1\B1Power Unit Failure Detected-Asserted /Deasserted!\A1L SEL on BMC WebUI.(similar to 142745) 

[Known issue]:
n/a
=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.12.0
=====================================================================
Version: 2.12.0
Release Date: 2013.1.16

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1) 2b2s2120.ima with checksum  0x7B7D915B

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2S_S2B]1. add "SET_PCI_CARD_PRESENT" command for PTAS.
[S2B]2. add the Coefficient for PTAS (Fan Speed Ctrl) according to the HDD qty and PCI Card.
[S2S]3. add the code to read the psu data (MFR_REVISION and FW_VERSION). (142341) 

[Change/modify/Remove]
[S2B_S2S]1. remove the filter for DIMM size and frq. of webui's component.(142215,142193)
[S2B_S2S]2. change the Entity ID and Entity Instance of "PSU Alert" sensor to 0xd0 and 0x01. (142372)
[S2B_S2S]3. modify Network Privilege description (142399) (Raincer)
[S2B_S2S]4. add to handle STATUS_IOUT/STATUS_TEMPREATURE event when SMBAlert is been triggered. (Keven)
[S2B_S2S]5. only recorded event log for system power core dropped. (Keven)
[S2B_S2S]6. change polling PSU_status time from 2s to 1s. (Keven)
[S2B_S2S]7. added define macro to enable or disable SMBAlert MASK. (Keven)
[S2B_S2S]8. it blinking fault LED if sensor type is voltage. (Keven)
[S2B_S2S]9. add power saving mode (Alan)
[S2B_S2S]10. Change the severity of "ME Firmware Health Event". (142367) 

[Bug Fixed]:
142399 S2B Base on 142061, after the ''No Access'' privilege is removed in the Help string, the number of Privilege should be 5, not 6, and description has typo. 
142372 S2B VMware 5.5 Certification Cert Test - Power Supplies Number Failed.(VMKernel Release Build 1331820) (same as S2S#141602)
142193 S2B RAS Memory DIMM information would show as ''Unknown'' in WebUI when set to Memory RAS Mode.
142341 S2S [DVT2]After update BMC Fw 2.10 to 2.11 , the PSU0/1 MFR Revision/Firmware Version will show N/A on BMC WebUi.
142215 S2S DIMM information would show ''Unknown'' on WebUI when set Memory to RAS Mode.(S2B:142193)
142367 S2S [DVT2] After update BIOS ,the Severity information will show critical on BMC WebUi.(same as standard BMC SPEC), but event level is too high.

[Known issue]:
1. Don't report the portion of cmc sensor.

=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.11.0
=====================================================================
Version: 2.11.0
Release Date: 2013.1.9

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1) 2b2s2110.ima with checksum  0x7BA3F602

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2B_S2S]1. add the filter condition for the event "PROCHOT# Assertions" of "CPUx_Therm_Sta" (ME).(141873)
[S2B_S2S]2. add the airflow sensor for PTAS.
[S2B_S2S]3. Web UI Code:add get PSU information (raincer)
[S2B_S2S]4. add NM event definition (raincer)(141585)
	event type 0x75 (OEM)
	event data 2: 
	=0x09 Firmware Exception
	=0x0A Flash Wear - Out Protection Warning
	=0x0C Invalid SCMP interface state
	=0x0D PECI over DMI interface error
	=0x0E MCTP interface error
[S2B]5. add code to "get PSU information"(MFR revision and FW version) at fw. 
[S2S]6. add some "MB type" for fan table of CMC.
 
[Change/modify/Remove]
[S2B_S2S]1. Modify the temp filter condition to 85 for the event MEM Hot.
[S2B_S2S]2. remove "No Access" from LDAP and Active Directory and update User Help page.(raincer)(142061)(142150)
[S2B_S2S]3. filter PM-bus alert signal if this signal is in 400us ~ 1000us.(keven)
[S2B_S2S]4. modify the UCT and LCT of "Volt_P3V_BAT" to 3.6v and 2.7v. (142059)(142103)
[S2B_S2S]5. modify sensor filter condition at webui dashboard.(raincer)
[S2B_S2S]6. Add to do power on delay 6s. it will wait Msghandler to be ready and delay 6s to do power on. (keven)(141408)
[S2B_S2S]7. Change to get DIMM temperature method through raw peci command. (keven)(142144)(142017)(142009)
[S2B_S2S]8. postpone 3 seconds to power on sysetm once BMC got the SYS_PWR_OK failure.(keven)
[S2B_S2S]9. add to restore system status if "SYS_PWROK failure" status is set by PCH when system was in S0 or S1.(keven)
[S2B_S2S]10. fix Alt key issue in Windows (Alt key will be transfered to the Windows)(raincer)
[S2B_S2S]11. reject Web account to login BMC by SSH(raincer)(142160)
[S2B_S2S]12. modify the bmc aux version to 0. (142025)(142003)(141998)
[S2B]13. remove the code to log detail psu event(OEM).(142177)
[S2S]14. it would report the wrong motherboard type to H8 sometimes.(keven)
[S2S]15. modify the PTAS outlet code.(141424)
[S2S]16. modify the UCT of Temp_Ambient_FP to 43. 

[Bug Fixed]:
142061 S2B Base on #141894, the privilege of No Access is removed, but the Help String is still mention the privilege of No Access. 
142059 S2B Run the Remote Power On / Off cycling for overnight will occur SPS FW Health error and Volt_P3V_BAT UCT.
142025 S2B BMC v2.10 version number is incorrect when flash BMC by WebUI and check the version under BIOS Setup. 
141873 S2B System recorded ''CPU1 Thermal Sta - PROCHOT# Assertions'' after PSU Redundancy Lost. 
142150 S2S The privilege of No Access is removed, but the Help String is still mention the privilege of No Access.(S2B ID 142061) 
142103 S2S [DVT AVL](PSU Chicony 1600W)After run system stress/idle system under RedHat 6.5 x86_64,the system will log ''Volt_P3V_BAT-Going High Asserted/Deasserted'' message on BMC WebUi.
142009 S2S [AVL] (Mezz 2308 card and LSI 9207-8e )BMC SEL will record ''CPUx Thermal Sta'' logs during run full system stress and CPU1/2 Temp always keep at 68 degree
142003 S2S BMC v2.10 version number is incorrect when flash BMC by WebUI and check ver under BIOS Setup. 
141998 S2S [BMC Sanity] After update BMC FW 2.09 to 2.10 and check BMC Fw version,the BMC Fw version will show 2.10.e4 in BIOS setup.
141424 S2S FSC SPEC (Temp_Outlet) is under definition (calculated by Intel PTAS) , plan to be ready by DVT2. 
142144 S2S Sometimes the Temp_DIMM sensor will show sub-zeno tempurature value on BMC WebUi.
142017 S2S The BMC SEL will log ''CPU0 Thermal Sta - TCC Activation'' & ''CPU1 Thermal Sta - TCC Activation'' when execute system stress under OS.(Windows 2012 R2/ RHEL 6.5 have same issue) 
141408 S2S After updated BMC Fw 2.06.00 to 2.07.00 , the system would log CMC_REP/FAN_TAB_STA Asserted/Deasserted on BMC WebUi. 
142160 S2S Connect to the SMASH with the WebUI Account and Password,the system should not be connected and should have error message.
141585 S2S ''SPS FW Health - undefined - undefined - Asserted'' generated after flash BIOS via WebUI, but Event Table Standard v1.6 doesn't define it. 
142177 S2B Unplugged the Power Cord will log BMC FW info - PSU1 - 0x7C - 0x03 - Asserted (Or 0x7C - 0x38, 0x7C - 0x00) and they are undefined in Event table1.8. 

[Known issue]:
1. Don't report the portion of cmc sensor.
2. the psu info at the dashboard of webui are n/a for s2s.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.10.0
=====================================================================
Version: 2.10.0
Release Date: 2013.12.27

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1) 2b2s2100.ima with checksum  0x7B9D0667

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
na.

[Change/modify/Remove]
[S2B_S2S]1. Modify the Fan reading cal method for PTAS.
[S2B_S2S]2. Modify the voltage threshold to +/-5%.
[S2B_S2S]3. Change the "CPU0/1 Thermal Sta" to "event only" type.
[S2B_S2S]4. Remove "No Access" from "Network Privilege".
[S2B]5. Add the more error event with OEM event data for PSU status and modify the QPMBusDev ddf.
[S2B]6. Change the sku3 & sku4 PID fan table.
[S2S]7. Change the Temp_Outlet reading source to ME/.
[S2S]8. Add the delay to monitor the HSC.
[S2S]9. Enabled i2c slave mode after message handler is in readiness.
[S2S]10. CommunicateWithCMCTask is changed to the first tick in PDK_TimerTask.
[S2S]11. According to the SKU type to filter the unnecessary hdd from WebUI.

[Bug Fixed]:
141894 S2B ESMS spec v.053 not defined the user privilege of 'No Access' but BMC web has this privilege. [Same with S2S 141690] 
141730 S2B [SDA]There is no PSU 12V voltage threshold event when voltage adjust to +/-6%. 
141690 S2S The BMC Standard SPEC ESMS v0.53 doesn't define ''No Access'' User privilege, but S2S BMC still have this User privilege. 
141679 S2S [DVT AVL](IB Mezz)After run AC cycles about 12hrs , the system will log BMC event ''BMC FW info-SKU - Chassis - Unavailability - Asserted''(BMC:2.07 pass) 
141225 S2S After update BMC Fw 2.05.00 to 2.06.00 and check Sensor Readings on BMC WebUi, all HDD0 to HDD23 sensor name shown in BMC WebUI(but no support HDD6-23) 

[Known issue]:
1. Don't report the portion of cmc sensor.
2. Will have Volt_P3V_BAT event.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.09.0
=====================================================================
Version: 2.09.0
Release Date: 2013.12.18

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1) 2b2s2090.ima with checksum  0x7BBEAB1B

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
na.

[Change/modify/Remove]
[S2B_S2S]1. fix the event string issue for sensor "CPU Thermal Status".
[S2B_S2S]1. fix the zero reading for temp sensor.
[S2B_S2S]1. modify display of the "power status".
[S2S] modify the QLM25062.ddf.
[S2S] change the entity id and instance of HSC0 Input.

[Bug Fixed]:
141605 S2B BMC Web UI display the ''Temp_Outlet,Temp_CPU_0,Temp_CPU_1,Temp_PCH'' Sensor reading are ''0?XC'' [Same as S2S : 141596]
141566 S2B Unplugged and plug in the PSU1 Power Cord and it will occurred CPU1 Thermal Sta Processor undefined - Asserted 
141596 S2S After update BMC FW 2.07 to 2.08 and check the status on BMC WebUi,the ''Temp_Outlet,Temp_CPU_0,Temp_CPU_1,Temp_PCH'' Sensor reading will show ''0?XC'' on BMC WebUi.
141420 S2S After update S2S BMC FW 2.07,the BMC Power restore policy does not follow the BMC standard SPEC v0.19 definition.


[Known issue]:
1. Don't report the portion of cmc sensor.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.08.0
=====================================================================
Version: 2.08.0
Release Date: 2013.12.12

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1) 2b2s2080.ima with checksum  0x7BC0B7CF

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2B_S2S]1. add the temp condition to filter the CPU_DIMM_HOT event.

[Change/modify/Remove]
[S2B_S2S]1. chang the power policy to "RestorePowerState".
[S2B_S2S]2. modify the QPI Error event string & "Memory correctable/Uncorrectable Error Event" and "Memory Correctable Error Log Disabled Event" for webui.
[S2B_S2S]3. modify unit1 to 0x81 of QMETEMP.ddf.
[S2B_S2S]4. remove the sel filter condition for type 0xc0 (for BIOS).
[S2B_S2S]5. modify sensor name of the CPU_DIMM_HOT to DIMM_HOT.
[S2B_S2S]6. (AppDevice+.c)reduce the delay time to improve Mesg performance.
[S2B_S2S]7. modify the temp ddf to support 2's complement.
[S2B]8. modify the PID algo. 
[S2S]9. add the code to support the "1023W" power into webui for CMC.

[Bug Fixed]:
141420 S2S After update S2S BMC FW 2.07,the BMC Power restore policy does not follow the BMC standard SPEC v0.19 definition.
141405 S2S The Fan table error SEL string was mismatch with Event table v1.4 definition.
140999 S2S After generate DIMM A1 ECC error, BMC SEL showed ''ECC DIMM G1''l , it should be slot A1 
141510 S2S Unplugged and plug in the PSU1 Power Cord and it will occurred CPU pochot and DIMM memory hot.(Same as S2B 141370) 
141479 S2B [SDA]BMC log occurred ''Processor #0x1c, Processor #0x1d, Unknown CPU_DIMM_HOT | | Asserted '' after disconnect AC power core.
141370 S2B Unplugged and plug in the PSU1 Power Cord and it will occurred CPU pochot and DIMM memory hot.
141306 S2B Memory ECC Error location report from SEL is not followed M/B DIMM Silkscreen.
141053 S2B After run the Memory Leak test for 48 hours, BMC has occurred abnormally SEL and cannot open Web UI. [But use ipmitool is workable.]
141494 S2B System recorded abnormal event ''Temp_Outlet'' when system idle under W2008R2SP1 overnight.


[Known issue]:
1. Don't report the portion of cmc sensor.

=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.07.0
=====================================================================
Version: 2.07.0
Release Date: 2013.12.05

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1) 2b2s2070.ima with checksum  0x7BBE9B69

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2B_S2S]1. add the "Reset Button pressed" event for Button sensor.
[S2B_S2S]2. add 4 sensors for CMC. SENSOR_NUM_REPEATER_TAB_STATUS_CMC:, SENSOR_NUM_FAN_TAB_STATUS_CMC, SENSOR_NUM_REPEATER_READY_STATUS_CMC &  SENSOR_NUM_LINKING_BOARD_STATUS_CMC.

[Change/modify/Remove]
[S2B_S2S]1. modify the mb thermal trip unc to 40 from 42.
[S2B_S2S]2. change the Sel severity of processor for ME.
[S2B_S2S]3. modify log description for sensor critical event (by Raincer).(remove space)
[S2B_S2S]4. modify the event string for DIMM XX ECC error.
[S2B_S2S]5. changed behavior by blinking fault LED.it will blinking fault LED when the event log from BIOS are "mem err/pcie err/post err" and severity is over than OK status.
[S2S]6. fix the hdd type issue for CMC.
[S2S]7. change the QPower and QLM25062 ddf.
[S2S]8. change the 1-based to 0-based for dimm name of component page of WebUI.
[S2S]9. change the event string "OCP" to "Over Current Protection" for PDB Event.
[S2S]10. modify the MDS content to fix the Temp_Ambient_FP problem.
[S2S]11. fix bug that the mb thermal trip don't work.
[S2S]12. change the sensor name of Temp_MB_Inlet to Temp_Inlet_MB.
[S2S]13. change the  CMC_SKU_TIMER_DUE_TIME to 20 from 15.
[S2S]14. remove the system mac0/1 string from th dashboard of webui.
[S2S]15. modify the ddf code to fix the bug which "HSC0 input" reading is wrong.

Bug Fixed:
141303 S2B Severity of ''TCC Activation - Asserted'' is not correct.
141253 S2B SEL doesn't logged reset event after pressing reset button. 
141104 S2S The order of BMC WebUI DIMM info doesn't meet HW SPEC ''Connector_color_Std_SPEC Ver0.8''. 
141046 S2S The S2S Fan Speed doesn't not follow S2S FSC SPEC R001 definition.  
141037 S2S After update BMC FW 2.05.0 and AC off/on , the system will log BMC event ''BMC FW info-SKU - Chassis - Unavailability - Asserted'' (BMC 2.04 passed) 
141017 S2S After generate CPU 0,1QPI error , but BMC SEL not correctly record this CPU0, 1 description 
140979 S2S After write wrong Fan table on X5M Chassis, the BMC will not alert '' Fan Table Error event asserted -State Asserted - Asserted'' 
140943 S2S POST Err inj test (ex. clear Password; information level log), Power button LED on X5M front panel would be blue/amber blinking(means system fault). 
140932 S2S The S2S BMC PDB event description ''OCP alert'' and Severity doesn't meet the Standard Event table v1.2 definition.
140294 S2S System MAC show ''Disable'' on BMC WebUI Dashboard.

[Known issue]:
1. Don't report the portion of cmc sensor.

=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.06.0
=====================================================================
Version: 2.06.0
Release Date: 2013.11.28

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1) 2b2s2060.ima with checksum  0x7BD0F2D0

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2B_S2S]1. Add new ddf.

[Change/modify/Remove]
[S2B_S2S]1. Change the channel 1 users 1 of Access Limit to 0x04.
[S2B_S2S]2. according the event table, change the sel severity of drive of WebUI.
[S2B_S2S]3. change the string to SSH from SMACH.
[S2B_S2S]4. add smbapp in .PRJ, so that it will add libsmb_dev depandency.(Keven)
[S2B_S2S]5. add i2c patch to work the block write-block read and Block Write/Read transactions.(Keven)
[S2B_S2S]6. add SMBUS alert mask for PSU. if the VIN-FAULT bit of "INPUT STATUS" is trigger and the corresponding bit in "SMBUS alert mask" not mask. BMC will disable it to avoid SMBUS alert.(Keven)
[S2B_S2S]7. changed the polling time of CPU_MEM_HOT from 3s to 1s.(Keven)
[S2B_S2S]8. Added delay time (1time * 2s) to do SMBAlert MASK.(Keven)
[S2B_S2S]9. Change the "Preserve Configuration Item" of WebUI from Authentication to Service.(filer the Authentication not Service).
[S2B_S2S]10. hdd sensor will show on the webui if hdd is n/a.
[S2B_S2S]11. add snmp string for invalid ipv4/ipv6 address.
[S2B_S2S]12. fix the dimm info when dimm ecc error occur.
[S2B_S2S]13. change the log sku event code.
[S2B_S2S]14. change the name of "CPUx Processor Hot" to "CPUx Thermal Sta".
[S2S]15. change to the sensor(#0xf9) from sensor(#0xee) for mb thermal trip.
[S2S]16. Change the Temp_MB_Inlet entity instance to 12 from 11.
[S2S]17. change the unct/uct to 40/45 for sensor "Temp_Ambient_FP".
[S2S]18. modify the event severity of webui for PDB Event.

Bug Fixed:
141046 S2S  The S2S Fan Speed doesn't not follow S2S FSC SPEC R001 definition. 
141044 S2S  It's strange that ''UNCT/UCT is 50/55'', but all of systems will shutdown automatically, when Sensor ''Temp_Ambient_BP0'' reached 45 degrees.The UNCT/UCT temp is higher than actual shutdown value. 
140999 S2S  After generate DIMM A1 ECC error, BMC SEL showed ''ECC DIMM G1''l , it should be slot A1  
140932 S2S  The S2S BMC PDB event description ''OCP alert'' and Severity doesn't meet the Standard Event table v1.2 definition. 
140723 S2S  [Olson][S2S]The Severity icon of SEL ''Rebuild/Remap is progress - Asserted'' is wrong, it shows ''Unspecified'' 
141027 S2S  "Preserve Configuration Item " is different btw. BMC Update page and ESMS specification definition. [Same as S2B 141026]
140903 S2S  Privilege of anonymous user on BMC WebUI is different to ESMS SPEC v0.51. 
141022 S2S  (1)During heating CPU process, BMC got logs were mismatch to Intel ME SPEC. (2)Standard BMC SPEC haven't define it yet. (For PROCHOT,Thermaltrip, TCC Activation event test)
141170 S2B  Set the SNMP Community Settings with invalid IPv6/IPv4 address will prompt a 'Undefined' dialog. 
141094 S2B  The HDD sensors are disappeared from Web UI Driver Slot filter. 
141026 S2B  Preserve Configuration Items in BMC Update page are mismatched with ESMS specification defined.
140908 S2B  Privilege of anonymous on BMC WebUI is different with ESMS SPEC v0.51 snapshot sample. [Same as S2S 140903]

[Known issue]:
1. Don't report the portion of cmc sensor.
2. The "HSC0 Input" reading is wrong.

=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.05.0
=====================================================================
Version: 2.05.0
Release Date: 2013.11.21

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1) 2b2s2050.ima with checksum  0x7BD973D6

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
n/a

[Change/modify/Remove]
[S2B_S2S]1. Modify the severity of HDD/DriveSlot.
[S2B_S2S]2. modify the SNMP function.
[S2B_S2S]3. Modify the Fan name.
[S2B_S2S]4. Enable the Delete SDR command.
[S2B_S2S]5. change the Privilege of "QUANTA_GET_BOARD_ID" command to "USER".
[S2B_S2S]6. Add the function to change the threshold of Temp_CPU_0 and Temp_CPU_1 by TjMax from CPU at runtime.
[S2B_S2S]7. Add the deasserted for PSU Alert event.
[S2B_S2S]8. modify the FRU event rule.
[S2S]9. change the name of "Temp_Exhaust" to Temp_Ambient_PCI". 
[S2S]10. Remove the "Temp_Inlet" sensor.
[S2S]11. modify the cmc code for mb type mapping.
[S2S]12. change HSC ddf.
[S2B]13. Modify the judge rule for dimm qty at WebUI. 
[S2B]14. Change the TjMax based value to 97 for 2U and to 99 for 1U.
[S2B]15. Change the sensor name Temp_Exhaust to Temp_PCI_Area.

[Bug Fixed]:
140911 S2B ''Delete SDR'' supporting of SDR Repository are mismatch to BMC FW SPECv008 [Same as S2S 140843] 
140783 S2B  Memory Information in Server Information will only display 16 slots. 
140705 S2B  The BMC WebUI will lost connection after setting SNMP Community String under Configuration/SNMP Community Settings [Same as S2S 140659] 
140828 S2B  [WebUI] Use Operator privilege to login and check Memory information in Server Information will prompt a dialog about ipmi error
140843 S2S  ''Delete SDR'' supporting of SDR Repository are mismatch to BMC FW SPECv008. 
140829 S2S  [WebUI] Use Operator privilege to login and check Memory information in Server Information will prompt a dialog about ipmi error [Same as S2B 140828] 
140723 S2S  [Olson][S2S]The Severity icon of SEL ''Rebuild/Remap is progress - Asserted'' is wrong, it shows ''Unspecified'' 
140659 S2S  [Olson][S2S]The BMC WebUI will be disconnect after setting SNMP under Configuration/SNMP Community Settings 
140585 S2S  [SDA]SEL show ''PSU Alert'' during AC interrupt test but no show ''PSU disalert'' when voltage is normal 

[Known issue]:
1. Don't report the portion of cmc sensor.
2. The "HSC0 Input" reading is wrong.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.04.0
=====================================================================
Version: 2.04.0
Release Date: 2013.11.15

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1) 2b2s2040.ima with checksum  0x7AB28EE2

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
n/a

[Change/modify/Remove]
[S2B_S2S]1. Remove the code of MG9086.
[S2B_S2S]2. EIP 140333:  fix "Set Management Controller Identify String" failed in NMCT test: pend to restart network service after sent this command
[S2B_S2S]3. modify the code about broadcast storm.
[S2B_S2S]4. Change the threshold for Volt_VR_CPU0 and Volt_VR_CPU1.
[S2B_S2S]5. Change the dram clk to 0x23 and i2c clock to 93k(except bus4(0-based)).
[S2B_S2S]6. Add the cpu offset for PID according TjMax.
[S2S]7. Add the "SKU_STATUS_CHASSIS_ERROR" event for X5M sku error.
[S2S]8. Modify the sel severity of WebUI for PDB Event.
[S2B]9. Remove the sensor "PDB event".
[S2B]10. Change the order of FRU id.

[Bug Fixed]:
140567	S2B	FRU Device ID sequential is not started based from 0. 
140386	S2B	When SUT booting to RHEL 6.4 uefi mode, BMC will log the Temp_DIMM_AB has occurred UNCT and UCT event. 

[Known issue]:
1. Don't report the portion of cmc sensor.

=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.03.0
=====================================================================
Version: 2.03.0
Release Date: 2013.11.11

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1) 2b2s2030.ima with checksum  0x7AB1BF9F

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2B_S2S]1. Add the "BUTTON" sensor and new event into "Power Unit".
[S2B_S2S]2. Add the prompt warming message when setting reserved IPV6 [2001::/32] as gateway address under WebUI.
[S2B_S2S]3. Add new sensor "CPU0 PRHOT" and "CPU1 PRHOT" for ME.
[S2S]4. Add new sensor "Temp_Ambient_FP" for CMC.
[S2S]5. Add OCP event into PDB event SDR.

[Change/modify/Remove]
[S2B_S2S]1. Add the string to the "BMC FW HEALTH" event sensor.
[S2B_S2S]2. Change the sensor number.
[S2B_S2S]3. Enable the SNMP function of WebUI.
[S2B]4. Enhance the PID code.
[S2B]5. Modify the MBThermalTrip sensor to SENSOR_NUM_TEMP_AMBIENT_1(0xee).
[S2B]6. Fix the PID bug.

[Bug Fixed]:
140292 S2S SUT will NOT prompt warning message(fail) when setting reserved IPv6 [2001::/32] as gateway address under BMC WebUI.
140305 S2B SUT will NOT prompt warning message(fail) when setting reserved IPv6 [2001::/32] as gateway address under BMC WebUI 	   [Same as S2S 140292]
140387 S2B The System Fans are always in full speed.

[Known issue]:
1. Don't report the portion of cmc sensor.

=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.02.0
=====================================================================
Version: 2.02.0
Release Date: 2013.11.7

AMI Subversion Revision: SP-X for AST2300 2011Q3

[Utility]
1. SOCFLASH (version v.1.09.02)

[Firmware Images]
1) 2b2s2020.ima with checksum  0x7AB670F0

[Note]
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2B_S2S]1. Add the "BUTTON" sensor and new event into "Power Unit".
[S2B_S2S]2. Add the prompt warming message when setting reserved IPV6 [2001::/32] as gateway address under WebUI.
[S2B_S2S]3. Add new sensor "CPU0 PRHOT" and "CPU1 PRHOT" for ME.
[S2S]4. Add new sensor "Temp_Ambient_FP" for CMC.
[S2S]5. Add OCP event into PDB event SDR.

[Change/modify/Remove]
[S2B_S2S]1. Add the string to the "BMC FW HEALTH" event sensor.
[S2B_S2S]2. Change the sensor number.
[S2B_S2S]3. Enable the SNMP function of WebUI.
[S2B]4. Enhance the PID code.
[S2B]5. Modify the MBThermalTrip sensor to SENSOR_NUM_TEMP_AMBIENT_1(0xee).

[Bug Fixed]:
140292 S2S SUT will NOT prompt warning message(fail) when setting reserved IPv6 [2001::/32] as gateway address under BMC WebUI.
140305 S2B SUT will NOT prompt warning message(fail) when setting reserved IPv6 [2001::/32] as gateway address under BMC WebUI 	   [Same as S2S 140292]
140387 S2B The System Fans are always in full speed.

[Known issue]:
1. Don't report the portion of cmc sensor.

=====================================================================
        S2B/S2S AST2300 BMC FW Release v2.01.0
=====================================================================
Version: 2.01.0
Release Date: 2013.10.29

AMI Subversion Revision: SP-X for AST2300 2011Q3

Utility:
1. SOCFLASH (version v.1.09.02)

Firmware Images:
1) 2b2s2010.ima with checksum  0x7C578DA6

Note:
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2S_S2B]1. Add the PCA9546 code into "Build" folder.

[Change/modify/Remove]
[S2B_S2S]1. Modify the oem command (0x1c) to support v1.2v for DDR4.
[S2B_S2S]2. Fix the bug of "reading dimm temp" code. 
[S2B_S2S]3. Modify the patch file.
[S2B_S2S]4. Change the UCT & LCT of Volt_VR_CPU0/1.
[S2S]5. Add the code(MG9094) to support sku0 and sku1.
[S2S]6. Modify the cmc version format.

Bug Fixed:
140216 S2B System record a lot of ''Volt_VR_CPU1'' event when let system idle under UEFI RHEL 6.4 x64. 
136730 S2B Some Temperature sensors are display ''NA'' in the BMC WebUI. 
135608 S2B QCILxDiag(QuickHWCheck_V107_1112) test item ''BMC'' failed. 
140173 S2S The BMC Self Test shows "FAILED" in BIOS Setup Utility.

Known issue:
1. Don't report the portion of cmc sensor.

=====================================================================
        S2B/S2S AST2300 BMC FW Release v1.12.0
=====================================================================
Version: 1.12.0
Release Date: 2013.10.21

AMI Subversion Revision: SP-X for AST2300 2011Q3

Utility:
1. SOCFLASH (version v.1.09.02)

Firmware Images:
1) 2b2s1120.ima with checksum  0x7C69A7EC

Note:
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2S_S2B]1. Add new sensor "BMC FW HEALTH" to all sku.
[S2S_S2B]2. Add feature "Add Hot Keys" for WebUi.
[S2S_S2B]3. Add the DCMDevice.c.patch to fix the problem for the NMCT 3.0.
[S2S]4. Add the 96-lib_arm_board_PCA9546.c to switch the PCA9546.

[Change/modify/Remove]
[S2B_S2S]1. remove always_en_alt_c.patch from ApplyPatch.sh.
[S2B_S2S]2. remove the support of setting timeout of ssh.
[S2B_S2S]3. change the bmc fw version format to meet si standard. 
[S2B]4. fix fp fru checksum bug.
[S2B]5. change the sensor device of Temp_Ambient_FP to TMP75 for sku0.
[S2B]6. modify WebUi Service below.
	i.remove Telnet
	ii.SSH only support port setting
	iii.remove Current State(Active/Inactive)

Bug Fixed:
n/a

Known issue:
1. Don't report the portion of cmc sensor.
2. only support sku1 for s2s.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v1.11.0
=====================================================================
Version: 1.11.0
Release Date: 2013.10.9

AMI Subversion Revision: SP-X for AST2300 2011Q3

Utility:
1. SOCFLASH (version v.1.09.02)

Firmware Images:
1) 2b2s1110.ima with checksum  0x7D70B0A0

Note:
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[ADD]
[S2S_S2B]1. Add the help string of "Sensor Events" for "Modify Event Filter entry" page.
[S2B]2. Add the code to avoid bmc hang when there are no fp fru.

[Change/modify/Remove]
[S2S_S2B]1. Change the monitor status of P1V05 to "DonNotMonitorOnStandby" and name to Volt_P1V05. 
[S2S_S2B]2. Remove the NIC failover function.
[S2S_S2B]3. Remove the VR update function from WebUI.
[S2S_S2B]4. According to the no:513973 v0.9 to change the PTAS code(PnmOemGetReading()).

Bug Fixed:
[S2B]
139431	BMC can't access after flash BMC FW (1.09/1.10) on S2B (occurred on 10G SKU only) 
139698	System recorded a lot of event ''Volt_P1V05_STBY'' in SEL during Power Cycling.(AC,DC,Warm Boot).
135585	The Help string of PEF - Modify Event Filter entry has mentioned about Event Severity but has no this function in 		the WebUI.
  
Known issue:
1. Don't report the portion of cmc sensor.
2. only support sku1 for s2s.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v1.10.0
=====================================================================
Version: 1.10.0
Release Date: 2013.09.16

AMI Subversion Revision: SP-X for AST2300 2011Q3

Utility:
1. SOCFLASH (version v.1.09.02)

Firmware Images:
1) 2b2s1100.ima with checksum  0x7D73A464

Note:
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

[Added]
[S2B_S2S]1. Add new sensor "BMC FW Info" to log sku in fru error and bmc rst caused by watchdog and bmc cold/warm reset,etc.
[S2B_S2S]2. Add new command QuantaGetBMCInfo_SNMP() (0x30 0x40)for SNMP.
[S2B_S2S]3. Add new sensor "PSU Alert" to log PMBUS alert.
[S2B_S2S]4. Add new sensor "MB Thermal Trip" to log MB thermal trip.
[S2B_S2S]5. Add the SEVERITY code to QuantaSelSeverity.h for WebUI event table.
[S2B_S2S]6. Add the OEM command "CMD_QUANTA_SET_ALTITUDE_LEVEL_NM(0x30 0xA0)" for PTAS.
[S2B_S2S]7. Stop monitor HDD status when the HDD_MONITOR_RETRY_COUNTER > 5.
[S2S]8. Add the "MB thermal trip" function.

[Change/modify/Remove]
[S2S_S2B]1. Modify the ddf "QHOT.ddf" to avoid log the status when PSU alert.
[S2S_S2B]2. Enable the DCMI configuration of PMC.
[S2S_S2B]3. Don't log ''CPU_PROC_HOT'' and ''CPU_MEM_HOT'' event when PSU alert.

Bug Fixed:
[S2S]
138677	When insert two different PSU(1600W and 1400W) into X5M system, the BMC didn't alert any warming SEL.
138503	When remove one Power Cord from PSU, it will log ''CPU_PROC_HOT'' and ''CPU_MEM_HOT'' event on BMC WebUI. 


Known issue:
1. User can't change the option for NIC failover, so need add the OEM command for NIC failover function.
2. Don't report the portion of cmc sensor.
3. only support sku1 for s2s.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v1.09.0
=====================================================================
Version: 1.09.0
Release Date: 2013.09.05

AMI Subversion Revision: SP-X for AST2300 2011Q3

Utility:
1. SOCFLASH (version v.1.09.02)

Firmware Images:
1) 2b2s1090.ima with checksum  0x7DA2024B

Note:
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

Added/Changed/Modify/Remove:
[ADD]
[S2S_S2B]1. add the aux versoin to the BMC FW version format of WebUI.
[S2S_S2B]2. add time zone function to WebUI.
[S2S]3. add aux verison to WebUI for CMC version.

[Change/modify/Remove]
[S2S_S2B]1. modify the hdd sensor number.
[S2S_S2B]2. improve the multi-sku function.
[S2S]3. modify the settable/readable of pdb sensor to 0x0f.

Bug Fixed:
n/a

Known issue:
1. User can't change the option for NIC failover, so need add the OEM command for NIC failover function.
2. Don't report the portion of cmc sensor.
3. only support sku1 for s2s.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v1.08.0
=====================================================================
Version: 1.08.0
Release Date: 2013.08.016

AMI Subversion Revision: SP-X for AST2300 2011Q3

Utility:
1. SOCFLASH (version v.1.09.02)

Firmware Images:
1) 2b2s1080.ima with checksum  0x85976E46

Note:
1. The released file 2b2sxxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

Added/Changed/Modify/Remove:
[ADD]
[S2S_S2B]1. Add the IPMI OEM command(0xfb) to get the VR version.
[S2S_S2B]2. Add the code to reading the FAN speed of zone and inlet temp for IPMI OEM command "OEM Get Reading"(0xe2) and PTAS.
[S2S_S2B]3. Add the sensor "Outlet Airflow Temperature" for PTAS.
[S2S]4. Add the sensor "PDB Event" for CMC.
[S2S]5. Add the CMC's PSU info on WebUI.


[Change/modify/Remove]
[S2S_S2B]1. Modify the code for reading DIMM temp reading from ME.
[S2S_S2B]2. Change the sensor type of "CPU_DIMM_VRHOT" to 0xc5.
[S2S_S2B]3. Change the sensor type of "CPU_DIMM_HOT" to 0xc6.
[S2S_S2B]4. Change the sensor name and entity id of "Thermal_Limit" to "DCMI Therm Limit" and 0x07.
[S2S_S2B]5. Change the calculation of HDD rep table's checksum.
[S2S_S2B]6. Change the bmc version format. 
[S2S_S2B]7. Remove uPNP.

Bug Fixed:
[S2S]
137806	S2S	After execute X5ChassisTestTool, the item ''HDD Repeater Table version'' was failed.
137767	S2S	After unplug Linking Board from X5M chassis and power on system, it will log the incorrect SEL related to sensor name 		"0xf8" on BMC WebUI.
137948	S2S	The BMC recorded the error SEL ''Temp_DIMM_CD Temperature Upper Critical - Going High (Reading:253 ?X C / 				Threshold:85 ?X C) - Asserted''.

Known issue:
1. User can't change the option for NIC failover, so need add the OEM command for NIC failover function.
2. Don't report the portion of cmc sensor.
3. At the page "BMC Firmware Update " of WebUI, the bmc fw version formate still don't change.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v0.07
=====================================================================
Version: 0.07
Release Date: 2013.08.01

AMI Subversion Revision: SP-X for AST2300 2011Q3

Utility:
1. SOCFLASH (version v.1.09.02)

Firmware Images:
1) 2b2s007.ima with checksum  0x85F34B6C

Note:
1. The released file 2b2sxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

Changed/Added/Modify:
[ADD]
[S2S_S2B]1. Add the "VR Update" function into WebUI.
[S2S_S2B]2. Add new sensor "Thermal_Limit" for DCMI 1.5.
[S2S_S2B]3. Add IPMI OEM command(0xB0) for mb thermal trip.
[S2S_S2B]4. Add the code to read cpu/dimm/pch temp reading from nmcmd.c.
[S2S_S2B]5. Add pid commands.(0x90 & 0x91)
[S2S_S2B]6. Add new file "NMCmd.h".
[S2S_S2B]7. Add the hdd event message into pop message window.
[S2S_S2B]8. Add the lc threshold for all power consumption sensors.
[S2S_S2B]9. Add the code to avoid ttyS2 to be opened but not closed for track 136678.

[Change/Modify]
[S2S_S2B]1. change the assertion event mask & deassertion event mask & setable/readable threshold mask of psu input.
[S2S_S2B]2. change the sensor number of inlet.
[S2S]3. change the Entity ID/Instance of sensor "HSC0 Input".
[S2S_S2B]4. change the temp sensor for mb thremal trip.
[S2S_S2B]5. change the 0-based to 1-based for "System MAC info" at dashboard.
[S2S_S2B]6. Modify the sensor order for webui. 
[S2S_S2B]7. Modify conmgr.c.patch.
[S2S_S2B]8. Modify DCMI code for variable name.
[S2S_S2B]9. Modify the command ID of CMD_QUANTA_SET_BIOS_UPDATE_CONFIG to 0x99 from 0x90.
[S2S_S2B]10. Modify the "AD login format" and PEF for WebUI's Help string.
[S2S]11. Modify the reading method for inlet & exhaust temp.

Bug Fixed:
[S2B]
136809	BMC WebUI - The AD login format is mismatched with the help string described.
136678	Run the MemoryLeak test and it will randomly lost connection with Virtual Device HDD / USB / Floppy
135585	The Help string of PEF - Modify Event Filter entry has mentioned about Event Severity but has no this function in the WebUI.

[S2S]
137289	It doesn't show the current value of PSU Consumption on BMC WebUI page "Dashboard".
137228	After AC on/off the X5M Chassis, BMC WebUI will show some abnormal SEL about ''HDD sensor''.
136907	BMC WebUI - The AD login format is mismatched with the help string described.(Same as S2B ID :136809)
136769	Run the MemoryLeak test and it will randomly lost connection with Virtual Device HDD / USB / Floppy (Same as S2B#136678)

Known issue:
1. User can't change the option for NIC failover, so need add the OEM command for NIC failover function.
2. Don't report the portion of cmc sensor.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v0.06
=====================================================================
Version: 0.06
Release Date: 2013.07.18

AMI Subversion Revision: SP-X for AST2300 2011Q3

Utility:
1. SOCFLASH (version v.1.09.02)

Firmware Images:
1) 2b2s006.ima with checksum  0x85EA7A29

Note:
1. The released file 2b2sxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

Changed/Added/Modify:
[ADD]
[S2S_S2B]1. Support DCMI 1.5 commands.
[S2S_S2B]2. Add the cv for adc(voltage). 
[S2S_S2B]3. Add the IPMI OEM command(0x17) to read the Device ID(0x02) and checksum(0x01) from CPLD.
[S2S_S2B]4. Add the hdd sensor/event support to WebUI.
[S2S]5. Add the code to read the hdd table from EEPROM.

[Change]
[S2S_S2B]1.change the default mode to background mode for reading cpld.
[S2S_S2B]2.change the entity ID & instance of Inlet and CPU and Baseboard temp for DCMI 1.5.
[S2B]3. change the setting of device of Temp_Ambient_FP to STTS2002.

[Modify]
[S2S_S2B]1. modify the RMII2 IO driving strength to 75pF loading(11b)
[S2S]2. modify the PSU Sensor Status MACRO.
[S2S]3. modify the behavior of power and fault LED.


Bug Fixed:
[S2B]
136643	Flash BIOS 1A06 via Web UI will halt at ''Checking image size and project name, please wait''
136612	SNMP only support if customer has requested, please remove the SNMP function
WebUI.

[S2S]
137227	It shows the incorrect PSU status on BMC WebUI.
137212	Update BIOS 1A07, check the power LED(on front panel or M/B rear side) is still off after system power on.
137172	[SDA]When system shutdown, Power LED of Front Panel is still light
137058	The MB Position was showed incorrect value on BMC WebUI Dashboard page.(only occurred on Node2,Node3)
137031	When power on system with critical SEL, the power/status LED is only green-blinking.
136515	[SDA]Sensor reading of P1V05_STBY voltage in WebUI is deviated to actual voltage on MB(over 2%)
137228	After AC on/off the X5M Chassis, BMC WebUI will show some abnormal SEL about ''HDD sensor''. 

Known issue:
1. User can't change the option for NIC failover, so need add the OEM command for NIC failover function.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v0.05
=====================================================================
Version: 0.05
Release Date: 2013.07.05

AMI Subversion Revision: SP-X for AST2300 2011Q3

Utility:
1. SOCFLASH (version v.1.09.02)

Firmware Images:
1) 2b2s005.ima with checksum  0x86459D31

Note:
1. The released file 2b2sxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

Changed/Added:
1.Modify the sensor Temp_CPU0 and Temp_CPU1 to Temp_CPU_0 and Temp_CPU_1.

2.Modify CPU_DIMM HOT to CPU_DIMM_HOT.

3.Modify CPU_DIMM VRHOT to CPU_DIMM_VRHOT.

4.Add the prefix "volt" to all voltage sansor.

5.Change the UCT and UNCT of TEMP for S2B.

6.Add the LCT for all Ambient sensor.

7.Add HDD sensor and monitor HDD status from MG908x.

8.Change the format for communication with CMC.

9.Add the command "CMD_QUANTA_GET_HDD_REPETER_TABLE" for X5M.

10.Change the name "X5M" to "CMC".

11.Add to command to control the fan speed by manual.

12.Add the FPEnable IPMI command.
13.Disable the MB thermal trip(45C).
14.Remove SNMP from WebUI.

Bug Fixed:
[S2S]
136588	The SEL will occur Temp_Exhaust Lower Non-Critical asserted/deasserted event during Share-NIC stress under Windows.
136417	The sensor reading of ''PSU Input'' display as N/A on BMC WebUI.
136886	Compare SDR file with S2B_S2S BMC FW Spec.rev003 and it has some sensor names are mismatched.(same as S2B ID:136696)

[S2B]
136696	Compare SDR file with S2B_S2S BMC FW Spec.rev003 and it has some sensor names are mismatched.




Known issue:
1. User can't change the option for NIC failover, so need add the OEM command for NIC failover function.
=====================================================================
        S2B/S2S AST2300 BMC FW Release v0.04
=====================================================================
Version: 0.04
Release Date: 2013.06.05

AMI Subversion Revision: SP-X for AST2300 2011Q3

Utility:
1. SOCFLASH (version v.1.09.02)

Firmware Images:
1) 2b2s004.ima with checksum  0x865980BF

Note:
1. The released file 2b2sxxx.ima is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file 2b2sxxx.ima_enc is used for:
	i. Use BMC WebUI to update.

Changed/Added:
1. Add the Temp_Ambient_BP1 and Temp_Ambient_BP2 sensor for s2s.
2. Add the Temp_Ambient_FP fors s2b.
3. Add the (GPIO_SLP_S3_N) Mechanism to avoid BMC log 0v of P1V05_STBY when power off.
3. Change the UCT and UNCT of TEMP for S2B.
4. Change the dos/windows/linux flash utility version to v.1.09.02.

Bug Fixed:
136231	S2B	Use privilege of OEM to check Serial Over Lan (Include Advanced setting) , SNMP setting and Preserve 
		Configuration page ,the columns are not gray out.
136230	S2B	Use privilege of Operator to check DNS , Serial Over Lan setting (include Advanced setting), 
		SNMP setting and the Preserve Configuration page , the page will not gray out.
136196	S2B	Power off system and update BIOS via BMC WebUI, BMC WebUI would disconnect after pressing ''OK'' to 
		uploadthe BIOS bin.(BMC IP was reachable when WebUI disconnected) [Same as S2S 136018]
136184	S2B	BMC WebUI - To set value of "Character Accumulate Interval" to "0" under [Serial Over LAN Advanced Settings], 
		WebUI would prompt a dialog ''IPMI command error 204''.
135892	S2B	System will hang during BMC online flash cycling stress in RHEL 6.4 x64(stress test under Windows is ok)
136190	S2S	To set value of "Character Accumulate Interval" to "0" under [Serial Over LAN Advanced Settings], 
		WebUI would prompt a dialog ''IPMI command error 204''.(Same as S2B#136184)
136164	S2S	The system will hang (onboard CATERR LED light) during BMC FW flash cycling stress over night.
136018	S2S	Power off system and update BIOS via BMC WebUI, BMC WebUI will be disconnect after 
		upload the BIOS bin file and press "OK".(But still could ping BMC IP address)
135993	S2S	After run BIOS FW update about 12hrs,sometimes the system will 
		log ''P1V05_STBY voltage Lower critical Asserted / Deasserted'' on BMC webUi.



Known issue:
1. User can't change the option for NIC failover, so need add the OEM command for NIC failover function.

=====================================================================
        S2B/S2S AST2300 BMC FW Release v0.03
=====================================================================
Version: 0.03
Release Date: 2013.05.15

AMI Subversion Revision: SP-X for AST2300 2011Q3

Utility:
1. SOCFLASH (version 1.08.00)
2. fwtool (version 0.07)

Firmware Images:
1) s2bs2s003.bin with checksum  0x8631E37D

Note:
1. The released file s2bs2sxxx.bin is used for:
	i. Use socflash.exe under DOS to update.
	ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.
2. The released file s2bs2sxxx.bin_enc is used for:
	i. Use BMC WebUI to update.

Changed/Added:
1. Remove utility from release package.
2. Remove some field/data from the release not.
3. Add the code for MB thermal trip (AMA requirement) (sensor number:0xBB's temp. over 45C will shutdown MB)
4. Add NIC failover function.

Bug Fixed:
135693	S2B	BMC WebUI - Server Identify Timeout column is empty
135614	S2B	BMC WebUI Dashboard Help string is lack description for BIOS Version, BMC Date & Time, BMC Chipset, System MAC Addresses
135588	S2B	The PEF - Modify Event Filter entry default setting has some empty value.
135585	S2B	The Help string of PEF - Modify Event Filter entry has mentioned about Event Severity but has no this function in the WebUI.
135342	S2B	[AST2300] WebUI - in "Server Identify" page, some titles color in HELP field are differ with other HELP page.
135396	S2S	The CPU model name on S2S BMC WebUI shows incorrect.
135386	S2S	The Socket name of DIMM slot shows incorrect on BMC WebUI "Component Information" page.


Known issue:
1. User can't change the option for NIC failover, so need add the OEM command for NIC failover function.

=====================================================================
        S2B/S2S AST2300 BMC FW Release v0.02
=====================================================================
Version: 0.02
Release Date: 2013.03.28

Hardware Platform: S2B/S2S Rev. X00 (or later)
AMI Subversion Revision: SP-X for AST2300 2011Q3
Quanta Subversion Revision: 14732
Associate Platform:
  BIOS Version: N/A

Utility:
1. SOCFLASH (version 1.08.00)
2. fwtool (version 0.07)

Firmware Images:
  1) s2bsxxxM.bin with checksum  0x8B61CD76

Note:
   1. The released file s2bsxxx.bin is used for:
      i. Use socflash.exe under DOS to update.
     ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.

   2. The released file s2bsxxx.bin_enc is used for:
      i. Use BMC WebUI to update.

Changed/Added:
  1. BMC FW for EVT Build.

Bug Fixed:
  N/A

Known issue:
  N/A



=====================================================================
        S2B/S2S AST2300 BMC FW Release v0.01
=====================================================================
Version: 0.01
Release Date: 2013.01.23

Hardware Platform: S2B/S2S Rev. X00 (or later)
AMI Subversion Revision: SP-X for AST2300 2011Q3
Quanta Subversion Revision: 13797
Associate Platform:
  BIOS Version: N/A

Utility:
1. SOCFLASH (version 1.08.00)
2. fwtool (version 0.07)

Firmware Images:
  1) s2bsxxxM.bin with checksum  0x8B8902EB

Note:
   1. The released file s2bsxxxM.bin is used for:
      i. Use socflash.exe under DOS to update.
     ii. Use flash writer to pre-program FW into flash before mount on MB in Factory.

   2. The released file s2bsxxx.bin_enc is used for:
      i. Use BMC WebUI to update.

Changed/Added:
  N/A

Bug Fixed:
  N/A

Known issue:
  N/A

PCIE special card list:
- LSI storage card:
	Card name	    Vender ID   Device  ID	Sub Vender ID	Sub Device ID
	9300-8e	        0x1000	    0x97        0x1000	        0x30A0
	9300-4i4e	    0x1000      0x97        0x1000	        0x30F0
	9207-8e	        0x1000      0x87        0x1000	        0x3040
	9206-16e	    0x1000      0x87        0x1000	        0x3070
	9260-4i	        0x1000      0x79        0x1000	        0x9260
	9280-4i4e       0x1000      0x79        0x1000	        0x9282
	9270-8i	        0x1000      0x5B        0x1000	        0x9270
	9286-8e	        0x1000      0x5B        0x1000	        0x9290

- Mellanox card:
	Card name       Vendor ID   Device ID	Subsystem ID    Subdevice ID
	MCX354A-FCBT    15b3        1003        0050            1003
	MCX354A-QCBT    15b3        1003        0028            1003
	MCX354A-TCBT    15b3        1003        0027            1003

- Intel card:
	Card name       Vender ID	Device ID	Sub Vender ID	Sub Device ID
	E10G42BTDA      8086	    10fb     	8086  	        3
	I350T4G1P20     8086	    1521	    8086	        00a1
	X540T2G1P5      8086	    1528	    8086	        001A

- Skyhawk:
	Card name       Vender ID	Device ID	Sub Vender ID	Sub Device ID
	Skyhawk-10G	    10df		0720		152D			89C1
	Skyhawk-40G     10df		0720		152D			89BC
	X540T2G1P5      8086		1528		8086			001A
	
